{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TOC RE6 Data","Sheet1","Pyrograms"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TOC RE6 Data","index":0,"n_rows":31,"n_cols":15,"rows_kept":31,"cut":false,"hidden":false,"merged":[[10,1,11,3],[28,0,28,5],[27,0,27,5],[10,5,11,13],[0,0,0,14],[18,0,19,0]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / RE6"]
[]
["Job Number:","15-0601"]
["Well Name:","Berea Project - Sunday Creek 1740"]
["Formation:","Berea/Cleveland/Sunberry"]
["Sample Type:","cuttings"]
["Sample Size:","20/40 mesh"]
["Instrumentation:","LECO C230 & Rock-Eval 6"]
[]
[]
[null,"Total Organic Carbon (TOC) Reference Standard Results",null,null,null,"Rock-Eval 6 (RE6) Reference Standard Results (IFP 160000)"]
[]
[null,"Date","TOC Result","% Recovery",null,"Date","S1 Result","S2 Result","S3 Result","Tmax Result","S1 % Recovery","S2 % Recovery","S3 % Recovery","Tmax % Recovery"]
[null,"2015-10-13",5.03,100.2,null,"2015-10-13",0.16,12.37,0.88,416,{"$f":"(G14/0.14)*100","v":114.28571428571428},{"$f":"(H14/12.43)*100","v":99.517296862429603},{"$f":"(I14/0.79)*100","v":111.39240506329114},{"$f":"(J14/416)*100","v":100}]
[]
[]
[]
["DATE","Depth Range","Ave. Depth","SAMPLE ID","S1 (mg/g)","S2 (mg/g)","S3 (mg/g)","Tmax (°C)","S1+S2","Calc. %Ro-Tmax","TOC (% wt)","HI","OI","PI","NOC"]
["2015-10-13","2394-2404",2399,1,null,null,null,null,null,null,1.34]
[null,"2404-2411",2407.5,2,0.61,1.96,0.75,432,2.57,0.61599999999999966,2.5499999999999998,76.862745098039227,29.411764705882355,0.23735408560311286,23.921568627450981]
[]
[]
["RE6 analysis not performed on samples with TOC values < 1.50%"]
["S1 = Volatile Total Petroleum Hydrocarbons (mg/g)"]
["S2 = Kerogen yield (mg/g)"]
["HI = Hydrogen Index"]
["PI = Production Index"]
["Calc. %Ro-Tmax = Calculated%VRo = 0.0180 x Tmax - 7.16 (Jarvie et al., 2001)"]
["NOC = Normalized Oil Content = (S1/TOC) x 100 (Jarvie and Baker, 1984)"]
[]
["LECO B"]

{"sheet":"Sheet1","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":true,"merged":[[0,1,0,2],[5,1,5,2],[10,1,10,2],[15,1,15,2]]}
[null,"HI 700 LINE"]
[null,"y","x"]
[null,0,0]
[null,300,42.85]
[]
[null,"HI 350 LINE"]
[null,"y","x"]
[null,0,0]
[null,280,80]
[]
[null,"HI 200 LINE"]
[null,"y","x"]
[null,0,0]
[null,160,80]
[]
[null,"HI 50 LINE"]
[null,"y","x"]
[null,0,0]
[null,40,80]

{"sheet":"Pyrograms","index":2,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / SRA"]
[]
["Job Number:",{"$f":"'TOC RE6 Data'!B3","v":"15-0601"}]
["Well Name:",{"$f":"'TOC RE6 Data'!B4","v":"Berea Project - Sunday Creek 1740"}]
["Formation:",{"$f":"'TOC RE6 Data'!B5","v":"Berea/Cleveland/Sunberry"}]
["Sample Type:",{"$f":"'TOC RE6 Data'!B6","v":"cuttings"}]
["Sample Size:",{"$f":"'TOC RE6 Data'!B7","v":"20/40 mesh"}]