{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Boone Co Coal 835"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6","7"]
["SAMPLE DEPTH","2747-2755","2775-2785","2785-2789","2829-2833","2833-2843","2843-2854","2854-2866"]
[]
["NON-CLAY FRACTION"]
["Quartz",38.261776908606116,23.930479644069543,28.12137711340598,29.83367717215393,37.496089421453647,31.48615316734201,28.891460488057785]
["K-Feldspar",0.70409977486527286,0.49306375838236405,0.21550582484943201,0.65113874019916484,0.19779249704554003,0.23369879752319228,0.27314061270642109]
["Plagioclase",6.3888426144175519,3.6845346388755487,4.4995394247013039,4.847065791353625,6.0843058381182109,5.1672440893700458,5.0620801941792566]
["Organic Carbon (TOC)",0.32400000000000001,3.39,2.52,0.23100000000000001,0.32900000000000001,0.33500000000000002,0.372]
["Apatite",1.0912830359305762E-2,0,0,0,0,0,0]
["Pyrite",0.69791107647050998,2.440159509392176,2.0172881642893992,0.24814801773704709,0.65665044947244855,0.23603562756855856,0]
["Marcasite",0,1.0984469938621739,0.47147987951604997,0,0,0,0]
["Calcite",0,0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0,0]
["Siderite",1.0512514515982565,0.26494876753923718,0.55525019082245475,1.9586197060541548,0.88184370882862373,1.3451755398733058,1.1271138350859153]
["Anatase",0.9197510028258632,0.69199424240088947,0.65056109670722795,0.66380080399362551,0.83425709982601703,0.86461562618940158,0.89310138121604055]
["TOTAL",{"$f":"SUM(B9:B19)","v":48.358545659142862},{"$f":"SUM(C9:C19)","v":35.993627554521929},{"$f":"SUM(D9:D19)","v":39.051001694291855},{"$f":"SUM(E9:E19)","v":38.433450231491548},{"$f":"SUM(F9:F19)","v":46.479939014744495},{"$f":"SUM(G9:G19)","v":39.667922847866521},{"$f":"SUM(H9:H19)","v":36.618896511245417}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.4803828283383469,8.9551719930734723,8.7065439634853199,6.1417285652197409,6.4782935807429176,6.1188513379653102,7.718576044666337]
["Illite+Mica",34.578447769130996,47.790874829451248,43.087887767043334,46.18809408369259,37.90456587522678,45.151172090935212,46.453613725522509]
["Chlorite",5.0051313749930024,3.0294573924819312,4.3609138990106118,4.6741991851778337,5.620549660253328,5.7508566703935404,5.5669821237525721]
["Kaolinite",4.5774923683947835,4.2308682304714091,4.7936526761688825,4.5625279344182674,3.516651869032505,3.3111970528394066,3.6419315948131583]
["TOTAL",{"$f":"SUM(B23:B26)","v":51.641454340857138},{"$f":"SUM(C23:C26)","v":64.006372445478064},{"$f":"SUM(D23:D26)","v":60.948998305708152},{"$f":"SUM(E23:E26)","v":61.566549768508438},{"$f":"SUM(F23:F26)","v":53.520060985255533},{"$f":"SUM(G23:G26)","v":60.332077152133465},{"$f":"SUM(H23:H26)","v":63.381103488754576}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":100},{"$f":"E27+E20","v":99.999999999999986},{"$f":"F27+F20","v":100.00000000000003},{"$f":"G27+G20","v":99.999999999999986},{"$f":"H27+H20","v":100}]
[]
["% Expandable Layers in I/S",14.863279830399961,11.829425936400071,11.69307295240003,13.124779284400006,15.476868258400032,16.158633178400009,15.647309488399969]
["% I/S to Illite in <1.0um Fraction",23.282285934186117,18.02625949004721,20.332041496889772,14.300626386946421,18.238882177654958,14.314081417210012,16.785125967390545]
["% Expandable I/S Layers in sample",1.115444271601103,1.096517377494947,1.0443809368928181,0.80795469377465767,1.0059465269576582,0.99204609685790968,1.2122590856048929]
[]
[]
["Comments"]