{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea Project - E J Berwind 6 920"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2984-2995","2995-3009","3009-3014","3032-3042","3042-3049","3049-3057"]
[]
["NON-CLAY FRACTION"]
["Quartz",28.239309260847346,24.070311237177229,26.086019122944712,34.415007409043866,36.07231581831288,43.253718509785628]
["K-Feldspar",0.90257003426701832,0.45817691312521192,1.0107039453936562,0.51521227962972049,8.1843173225362942E-2,0.43732140482057341]
["Plagioclase",5.1930608408032466,4.0582518129213705,3.5514267650383009,5.0521278431361889,5.6821067215337422,7.4315460378777827]
["Organic Carbon (TOC)",0.45100000000000001,0.92800000000000005,2.11,0.23200000000000001,0.20599999999999999,0.21099999999999999]
["Apatite",0,0,0,0,0,0]
["Pyrite",0.50964193531955992,1.6987144150653266,1.9088246733140077,0.32869414931889929,0.22175494632789136,0.20861441218629972]
["Marcasite",0,0,0,0,0,0]
["Calcite",0,0,0,0,0,0]
["Dolomite",0,0,0,7.4514184204016879E-3,0,0]
["Siderite",1.420832240566209,0.41560047064131278,0.30995653788999361,1.4842378818949948,0.91781935832612715,0.63391341438143556]
["Anatase",0.81353339006977266,0.69782061931445127,0.59396328833861223,0.7426116239327285,0.80719398793493624,0.77486155133570622]
["TOTAL",{"$f":"SUM(B9:B19)","v":37.529947701873148},{"$f":"SUM(C9:C19)","v":32.3268754682449},{"$f":"SUM(D9:D19)","v":35.570894332919288},{"$f":"SUM(E9:E19)","v":42.777342605376809},{"$f":"SUM(F9:F19)","v":43.989034005660947},{"$f":"SUM(G9:G19)","v":52.950975330387422}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",8.5155160432670058,9.9780422138020093,10.808185778444146,7.0070272875777562,7.113154444640009,8.3186413885021686]
["Illite+Mica",43.664502822656758,50.245980513674674,47.057910114152271,41.323466024834943,39.484667050131243,31.002533915631744]
["Chlorite",5.1673944734048787,2.8597971030333773,2.6019012204787635,6.2612804270857492,5.2759548436390196,4.8499357038519655]
["Kaolinite",5.1226389587982117,4.5893047012450268,3.9611085540055448,2.6308836551247539,4.1371896559287702,2.8779136616266965]
["TOTAL",{"$f":"SUM(B23:B26)","v":62.470052298126852},{"$f":"SUM(C23:C26)","v":67.673124531755093},{"$f":"SUM(D23:D26)","v":64.429105667080734},{"$f":"SUM(E23:E26)","v":57.222657394623205},{"$f":"SUM(F23:F26)","v":56.010965994339045},{"$f":"SUM(G23:G26)","v":47.049024669612585}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":100.00000000000003},{"$f":"E27+E20","v":100.00000000000001},{"$f":"F27+F20","v":100},{"$f":"G27+G20","v":100}]
[]
["% Expandable Layers in I/S",14.829191584400064,10.943131540400032,12.463467312000011,11.488543476399968,14.181514910399983,10.874955048400011]
["% I/S to Illite in <1.0um Fraction",19.205567977848698,18.464175443360261,19.925147768703191,18.715462955272464,18.641233804868051,24.59929866216649]
["% Expandable I/S Layers in sample",1.268503137606996,1.1021381264262327,1.3761106359348454,0.806877331746231,1.0108353790472395,0.90656135609857746]
[]
[]
["Comments"]
[]
[]
["Sample #3 (3009-3014ft) did not have enough resolution with normal XRD runs to determine"]
["clay expandability. Approximate average was used (highlighted in orange)."]