{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":8,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea Project - Little Coal Land Co. 1340"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6","7"]
["SAMPLE DEPTH","2200-2210","2210-2220","2220-2230","2280-2290","2300-2310","2310-2320","2320-2330"]
[]
["NON-CLAY FRACTION"]
["Quartz",33.998369233782171,34.535605755069867,29.665666879091408,26.059356991468235,25.131103990485467,26.52213227650952,28.260191143555179]
["K-Feldspar",1.0533943539350754,0.5798103786086275,0.57895558294314964,1.1534815688687738,0.78420307920810817,0.651319200435995,0.55163571674039924]
["Plagioclase",5.2285098726071038,6.5389584249925683,5.5116412794832179,4.7788826555277764,4.5677650172978117,5.0772938659380866,5.0527962465797094]
["Organic Carbon (TOC)",0.49199999999999999,0.48,0.64300000000000002,0.27200000000000002,0.221,0.20599999999999999,0.23699999999999999]
["Apatite",0,0,1.7245643104048389E-2,0,0,0,0]
["Pyrite",0.44580030595284675,0.43843578340813721,0.49750527392119998,0.25630075609287056,0.26401140217086067,0.11472549830118531,0.23521752389990494]
["Marcasite",0,0,0,0,0,0,0]
["Calcite",0.36969739866219736,0,0,0.50420185513595872,0,0,0]
["Dolomite",0,0,0,0,0,0,0]
["Siderite",0.21577710384652121,0.66498656017182523,0.21342758593494884,0.70017685103442395,0.81507140782509235,0.80880097316764177,0.54463220532520462]
["Anatase",0.73311058011900143,0.67388215043141009,0.83145772233047865,0.90689143653814364,0.80319548070183089,0.72644711087742009,0.66758371325301857]
["TOTAL",{"$f":"SUM(B9:B19)","v":42.536658848904914},{"$f":"SUM(C9:C19)","v":43.911679052682437},{"$f":"SUM(D9:D19)","v":37.958899966808445},{"$f":"SUM(E9:E19)","v":34.631292114666181},{"$f":"SUM(F9:F19)","v":32.586350377689172},{"$f":"SUM(G9:G19)","v":34.106718925229856},{"$f":"SUM(H9:H19)","v":35.549056549353416}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",9.4019261036005499,10.454502857635644,6.3956109218282187,11.984870509403285,9.0774361963636583,11.467742285928168,9.5183448160820667]
["Illite+Mica",39.695253850742901,36.826375884142955,45.92663267904306,45.571634093157719,48.759174577952685,45.505400266345511,46.637831044176849]
["Chlorite",3.2384797553485711,3.5568498204836256,4.1538850076101879,4.0145863552126011,5.0585966761479426,4.6933431981794502,4.483521133656363]
["Kaolinite",5.1276814414030749,5.2505923850553424,5.5649714247100937,3.7976169275602065,4.5184421718465453,4.2267953243170284,3.8112464567313071]
["TOTAL",{"$f":"SUM(B23:B26)","v":57.463341151095101},{"$f":"SUM(C23:C26)","v":56.08832094731757},{"$f":"SUM(D23:D26)","v":62.041100033191555},{"$f":"SUM(E23:E26)","v":65.368707885333819},{"$f":"SUM(F23:F26)","v":67.413649622310828},{"$f":"SUM(G23:G26)","v":65.893281074770158},{"$f":"SUM(H23:H26)","v":64.450943450646577}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100.00000000000001},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":100},{"$f":"E27+E20","v":100},{"$f":"F27+F20","v":100},{"$f":"G27+G20","v":100.00000000000001},{"$f":"H27+H20","v":100}]
[]
["% Expandable Layers in I/S",14.420132632400055,16.056368440399979,12.579367348399956,15.988191948399958,15.442780012400021,16.942662836400018,14.795103338400054]
["% I/S to Illite in <1.0um Fraction",21.170812925996461,24.54854103578856,14.243784464228016,24.443144922669958,19.259644882450615,23.864821098516138,19.775904634529727]
["% Expandable I/S Layers in sample",1.3624735841735756,1.6867097040133876,0.80973398153241349,1.9213902833813745,1.404913361098439,1.9469516308115526,1.4115944304447405]
[]
[]
["Comments"]