{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - M H Burdette 1 1192"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4"]
["SAMPLE DEPTH","2199-2212","2212-2225","2254-2269","2269-2275"]
[]
["NON-CLAY FRACTION"]
["Quartz",28.135972079623137,28.758641581353388,33.863772439901503,32.902852602475967]
["K-Feldspar",0.2935645249889407,0.21434899853744632,0.31330948376150908,0.28468521658039858]
["Plagioclase",3.7852520324204098,4.6600879220147204,4.9680645947660071,5.5480826959214946]
["Organic Carbon (TOC)",2.5,2.2599999999999998,0.215,0.65500000000000003]
["Apatite",0,0,0,0]
["Pyrite",1.0824579971116879,1.3627051386975142,0.30234765488994469,0.4958982032938673]
["Marcasite",0,0,0,0]
["Calcite",0,0,0,0]
["Dolomite",0,0,0,0]
["Siderite",0.31184029818783948,0.39582905214068409,0.82903127833421153,0.72306864415136896]
["Gypsum",0.32126905844375059,0.33875583896336409,0,0]
["Anatase",0.62080290301312202,0.54701109031542894,0.75443937242737091,0.80250795013623388]
["Jarosite",1.1299370965627755,1.4369795057488177,0,0]
["TOTAL",{"$f":"SUM(B9:B21)","v":38.181095990351672},{"$f":"SUM(C9:C21)","v":39.974359127771358},{"$f":"SUM(D9:D21)","v":41.245964824080545},{"$f":"SUM(E9:E21)","v":41.41209531255933}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",10.534735833351885,11.324681281649323,5.5290342336726033,5.5459325589708017]
["Illite+Mica",43.659151252372759,40.80050633188025,43.067017634706254,41.086134336469655]
["Chlorite",2.9041261085726013,2.7911927414861974,5.311623354930969,4.2119075525770366]
["Kaolinite",4.7208908153510833,5.1092605172128751,4.8463599526096388,7.7439302394231975]
["TOTAL",{"$f":"SUM(B25:B28)","v":61.818904009648321},{"$f":"SUM(C25:C28)","v":60.025640872228649},{"$f":"SUM(D25:D28)","v":58.754035175919462},{"$f":"SUM(E25:E28)","v":58.587904687440698}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":100},{"$f":"C29+C22","v":100},{"$f":"D29+D22","v":100},{"$f":"E29+E22","v":100.00000000000003}]
[]
["% Expandable Layers in I/S",9.8523076683999307,9.6818664383999931,14.215603156399993,16.329074408399947]
["% I/S to Illite in <1.0um Fraction",23.27778688778475,24.088768884554248,14.326801499849608,13.77441775420138]
["% Expandable I/S Layers in sample",1.0645277808769262,1.1217930389439044,0.78767907505175994,0.91157023926118197]
[]
[]
["Comments"]