{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - UFG Min TR 28 1327"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2320-2329","2329-2342","2342-2355","2355-2366","2396-2405","2405-2412"]
[]
["NON-CLAY FRACTION"]
["Quartz",29.791353604206936,41.022589173149761,28.347791779466508,40.482643008084615,38.775003830059518,52.083198249004298]
["K-Feldspar",1.2025227965102399,0.13270439966207559,0.12450944402651243,0.48390259591429724,0.97851709400148557,0.38697727997820258]
["Plagioclase",5.3967024742498921,7.1223726550525877,4.7315940766668412,3.3609590162168219,5.602420197877656,7.7810192978342645]
["Organic Carbon (TOC)",0.56499999999999995,0.56999999999999995,2.7,2.74,0.27500000000000002,0.46400000000000002]
["Apatite",0,0,0,0,0,0]
["Pyrite",0,0.33169327989214975,1.9280388854713655,1.5860903116808795,0.20931944365213934,1.2309801952847099]
["Marcasite",0,0,0.71370329044254954,0.84531396575015427,0,0]
["Calcite",0,0,0,0.94083602140261946,0,1.4573674477841312]
["Dolomite",0,0.45092371539579112,0,0,0,0.27217311935247207]
["Siderite",0.49429204319369791,1.648377179789499,0.39839646961780234,0.13406123641299794,0.58879388907167896,1.1628343567117332]
["Gypsum",0,0,0.42822197426552971,0.29696826650925051,0,0]
["Anatase",0.84202076345887855,0.3196119113612883,0.53347532108009488,0.56293631967117308,0.80400465366173124,0.35283433625616006]
["TOTAL",{"$f":"SUM(B9:B20)","v":38.291891681619639},{"$f":"SUM(C9:C20)","v":51.598272314303145},{"$f":"SUM(D9:D20)","v":39.905731241037209},{"$f":"SUM(E9:E20)","v":51.433710741642805},{"$f":"SUM(F9:F20)","v":47.233059108324206},{"$f":"SUM(G9:G20)","v":65.191384282205973}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.9284687904803617,10.722164195610986,12.07335532716008,6.8097358509510126,4.9446119581318779,5.2077325278012996]
["Illite+Mica",43.684939992595652,31.234433861986286,41.381311131589477,37.60689158640038,40.309326077396577,24.579172681755562]
["Chlorite",3.4616474496785394,1.4419235602239064,3.1661261322666139,1.7361435116008992,4.107302066807172,2.4543469876869217]
["Kaolinite",6.6330520856257911,5.0032060678756576,3.4734761679466231,2.413518309404902,3.4057007893401665,2.5673635205502463]
["TOTAL",{"$f":"SUM(B24:B27)","v":61.70810831838034},{"$f":"SUM(C24:C27)","v":48.401727685696841},{"$f":"SUM(D24:D27)","v":60.094268758962791},{"$f":"SUM(E24:E27)","v":48.566289258357195},{"$f":"SUM(F24:F27)","v":52.766940891675794},{"$f":"SUM(G24:G27)","v":34.808615717794027}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":99.999999999999972},{"$f":"C28+C21","v":99.999999999999986},{"$f":"D28+D21","v":100},{"$f":"E28+E21","v":100},{"$f":"F28+F21","v":100},{"$f":"G28+G21","v":100}]
[]
["% Expandable Layers in I/S",20.76054638840003,13.499749990400005,10.397719604399981,12.102131904400039,16.874486344399998,11.352190492400041]
["% I/S to Illite in <1.0um Fraction",16.712688749103009,26.684565402748689,25.920411492830535,16.711454121398006,12.817997635133645,19.451069732268881]
["% Expandable I/S Layers in sample",1.6553461468672948,1.4557632102661842,1.2901887294563137,0.84734034034886885,0.83667873618303656,0.5939476339120352]
[]
[]
["Comments"]