{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - COL Gas Trans 1821"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","1863-1870","1883-1890","1910-1922","1936-1950","1950-1965","1965-1975"]
[]
["NON-CLAY FRACTION"]
["Quartz",30.722040556435516,30.15453504352195,43.336286677439759,44.31070961788916,43.05112242461783,48.179716436051962]
["K-Feldspar",0.75978535809794545,0.35512148054202447,0.31301516973512566,0.80260395236890003,0.80875848825130681,0.83940752108848127]
["Plagioclase",4.8790052230857954,4.361456438385396,5.6008219879877084,6.9671333114503433,6.6716696511684299,8.6129552595174292]
["Organic Carbon (TOC)",0.91,2.3199999999999998,1.71,1.36,1.6,1.08]
["Apatite",5.1765517584434623E-2,0,0,0,0,0]
["Pyrite",1.8761112154731927,1.193016276663978,1.0173967095985117,0.89824124148882811,0.70606878218362723,1.3554311750363552]
["Marcasite",0,0,0,0,0,0]
["Calcite",0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0]
["Siderite",0.67437841707569968,0.30777707402099319,0.24593243248334906,0.16533116713446991,0,0.24952737927204841]
["Gypsum",0,0,0,0.23547777247841808,0.2649099932694004,0]
["Barite",0,0.72912116399362936,0,0,0,0]
["Anatase ",0.6391683932621951,0.45018721448068666,0.49043270770588698,0.37654277293094962,0.41361461285081041,0.34428132341552242]
["Jarosite ",0.98631186530620529,0.59018810080384809,0,0,0,0]
["TOTAL",{"$f":"SUM(B9:B22)","v":41.498566546320987},{"$f":"SUM(C9:C22)","v":40.461402792412507},{"$f":"SUM(D9:D22)","v":52.713885684950341},{"$f":"SUM(E9:E22)","v":55.116039835741056},{"$f":"SUM(F9:F22)","v":53.516143952341402},{"$f":"SUM(G9:G22)","v":60.661319094381795}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",11.209464721731269,13.223666293689305,6.3267250478913963,7.6367677853396856,5.6768931526926201,5.9648134502073527]
["Illite+Mica",39.471981885775371,41.811442263036426,35.011921511213657,31.966384356312339,34.65633590602377,28.80870479940857]
["Chlorite",2.5849530695605725,1.715738985380505,1.511065548292291,2.1676883067925443,3.2045173724607618,1.9084044876755479]
["Kaolinite",5.2350337766118056,2.7877496654812606,4.436402207652308,3.1131197158143658,2.9461096164814267,2.6567581683267312]
["TOTAL",{"$f":"SUM(B26:B29)","v":58.50143345367902},{"$f":"SUM(C26:C29)","v":59.538597207587493},{"$f":"SUM(D26:D29)","v":47.286114315049652},{"$f":"SUM(E26:E29)","v":44.88396016425893},{"$f":"SUM(F26:F29)","v":46.483856047658584},{"$f":"SUM(G26:G29)","v":39.338680905618205}]
[]
["GRAND TOTAL",{"$f":"B30+B23","v":100},{"$f":"C30+C23","v":100},{"$f":"D30+D23","v":100},{"$f":"E30+E23","v":99.999999999999986},{"$f":"F30+F23","v":99.999999999999986},{"$f":"G30+G23","v":100}]
[]
["% Expandable Layers in I/S",11.045396278399949,12.17030839640006,13.806544204399984,11.590808214399999,9.7841311764000238,11.69307295240003]
["% I/S to Illite in <1.0um Fraction",25.723105315587908,25.783505611229106,16.373923829514926,22.006275757801699,17.333240144091175,19.174758279525811]
["% Expandable I/S Layers in sample",1.2495002514912312,1.6475849398574878,0.88869884060227067,0.8973673030999646,0.56446613089788311,0.70508490518329447]
[]
[]
["Comments"]