{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - UFG Mineral TR 737"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2440-2450","2460-2470","2470-2480","2560-2570","2580-2590","2590-2600"]
[]
["NON-CLAY FRACTION"]
["Quartz",31.786884131350018,31.552093365929746,33.743502718300149,26.873911751824206,40.741746690534193,46.704459631710058]
["K-Feldspar",0.47131734270080727,0.50984947782212908,0.17955315401757771,0.13146022686466394,0,0.15625979602287796]
["Plagioclase",5.3085983189677846,3.92467238049232,6.8832370459846262,3.2801635129066979,8.0106392236334649,7.5826983339999838]
["Organic Carbon (TOC)",0.40100000000000002,0.58699999999999997,2.08,0.23599999999999999,1.32,2.0699999999999998]
["Apatite",0.38430381422395482,0.28082195462019038,0,0,0,0]
["Pyrite",0.42994641198057632,1.1410362864659098,2.0114784231621887,0,0.77732645855344207,0.84520197286357845]
["Marcasite",0,0,0.39252501300485459,0,0,0]
["Calcite",0.41132523978237823,0.838072196686522,1.1985890681140132,0,0.40904361333415051,0.99284671501587818]
["Dolomite",0,0,0,0,0,0.23155369101590445]
["Siderite",2.0335415559617576,0,0.32152176800356563,2.4204925465547711,0.31262193840724678,0.38990711836648206]
["Gypsum",0,0,0.30296615113689396,0,0.14192442716919934,0]
["Anatase ",0.78669111052457175,0.39894556148400068,0.40396968460065746,0.69776023378124408,0.39179360351433401,0.51301761769121901]
["Jarosite ",0.81032646553323207,1.6097265754390573,0.82157937903913525,0,0,0]
["TOTAL",{"$f":"SUM(B9:B21)","v":42.82393439102507},{"$f":"SUM(C9:C21)","v":40.84221779893987},{"$f":"SUM(D9:D21)","v":48.338922405363661},{"$f":"SUM(E9:E21)","v":33.639788271931586},{"$f":"SUM(F9:F21)","v":52.105095955146034},{"$f":"SUM(G9:G21)","v":59.485944876685984}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",8.0199096963102452,14.223860470303066,13.032198134164943,10.232909714412051,7.9804110416000862,4.294914241993677]
["Illite+Mica",40.801613912384383,42.29850702707391,35.181602597774997,44.459106310286259,35.139359453394768,30.174887116111822]
["Chlorite",1.8052918413825079,1.3085597962415314,1.0802509722950953,2.3994403261308892,2.0633170537932357,2.3319317375826705]
["Kaolinite",6.5492501588977703,1.3268549074416198,2.3670258904012758,9.2687553772392111,2.7118164960658859,3.7123220276258482]
["TOTAL",{"$f":"SUM(B25:B28)","v":57.176065608974902},{"$f":"SUM(C25:C28)","v":59.15778220106013},{"$f":"SUM(D25:D28)","v":51.661077594636311},{"$f":"SUM(E25:E28)","v":66.360211728068407},{"$f":"SUM(F25:F28)","v":47.894904044853973},{"$f":"SUM(G25:G28)","v":40.514055123314016}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":99.999999999999972},{"$f":"C29+C22","v":100},{"$f":"D29+D22","v":99.999999999999972},{"$f":"E29+E22","v":100},{"$f":"F29+F22","v":100},{"$f":"G29+G22","v":100}]
[]
["% Expandable Layers in I/S",13.261132268400047,12.13622015040005,10.943131540400032,18.987957596399951,14.079250172400066,17.488074772400068]
["% I/S to Illite in <1.0um Fraction",19.789928147603508,29.443823833054338,29.336964485813123,21.259839860925329,21.276331607795274,14.010469633983142]
["% Expandable I/S Layers in sample",1.0678127618087958,1.7364318756719017,1.4564242079526435,1.9476169334133073,1.1386117099034392,0.76697417956735847]
[]
[]
["Comments"]