{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Jackson Machne & Electric 774"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2807-2823","2823-2840","2840-2852","2920-2935","2935-2946","2946-2957"]
[]
["NON-CLAY FRACTION"]
["Quartz",31.767353703123497,32.303067338778106,30.01396317445176,37.231977345281742,37.033245739187684,40.234564937990974]
["K-Feldspar",0.19653655270730216,0.26356902581854408,0.90380059544206393,0.34174484193784155,0.20344302375018006,0.19593588227757811]
["Plagioclase",4.4345720987700465,4.7915096437183147,4.2151481994286986,6.0722289343113207,5.789945173142681,6.4834315839952925]
["Organic Carbon (TOC)",0.93700000000000006,3.33,3.04,4.74,5.77,3.62]
["Apatite",0.41776490589912807,0.12843217283916786,0.15569242925778271,0,0,0]
["Pyrite",2.379977437318245,1.7351342271548551,2.2300647372261673,1.6641999236921703,2.0578336400099073,2.0437114387958495]
["Marcasite",0,0.25745137722978456,0.46418661895923152,0,0,0]
["Calcite",0,0.57611327935477252,0.37948569094348095,0,0.40959553000052845,0.70124038613294226]
["Dolomite",0,0,0,0,0,0.3319668577592636]
["Siderite",0.33527614161189684,0.23374602537392203,0.25314238399970718,0.19129719003630072,0.1632014195468621,0.19983748160886552]
["Anatase",0.51521517769477942,0.4667735617278122,0.49497372671555373,0.63521926129344608,0.5346161123821046,0.38384757694088956]
["Jarosite",1.1480034283545986,0,0,0,0,0]
["TOTAL",{"$f":"SUM(B9:B20)","v":42.131699445479491},{"$f":"SUM(C9:C20)","v":44.085796651995274},{"$f":"SUM(D9:D20)","v":42.150457556424449},{"$f":"SUM(E9:E20)","v":50.87666749655282},{"$f":"SUM(F9:F20)","v":51.961880638019963},{"$f":"SUM(G9:G20)","v":54.194536145501651}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",9.7714357877444904,8.9919707422169051,8.4887253355720595,6.7360573215541235,5.439082325338525,5.385513060544409]
["Illite+Mica",41.067192340601835,43.30524228332213,44.653156757288599,36.400748652598345,36.813075272299713,35.161067366920989]
["Chlorite",2.5753499043311847,1.9906345982825211,2.0639841038490663,2.9800827060504762,2.8826900919331537,2.3003846698778423]
["Kaolinite",4.4543225218429798,1.626355724183165,2.6436762468658364,3.0064438232442487,2.9032716724086947,2.9584987571551271]
["TOTAL",{"$f":"SUM(B24:B27)","v":57.868300554520495},{"$f":"SUM(C24:C27)","v":55.914203348004719},{"$f":"SUM(D24:D27)","v":57.849542443575558},{"$f":"SUM(E24:E27)","v":49.123332503447187},{"$f":"SUM(F24:F27)","v":48.038119361980087},{"$f":"SUM(G24:G27)","v":45.80546385449837}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":99.999999999999986},{"$f":"C28+C21","v":100},{"$f":"D28+D21","v":100},{"$f":"E28+E21","v":100},{"$f":"F28+F21","v":100.00000000000006},{"$f":"G28+G21","v":100.00000000000003}]
[]
["% Expandable Layers in I/S",11.965778920399998,17.692604248400016,12.374837872400008,14.590573862399879,15.885927210400041,21.953634998399934]
["% I/S to Illite in <1.0um Fraction",22.070702056664711,19.0485058070959,18.766136139830913,18.360584675669809,15.097779183344185,15.096573794149501]
["% Expandable I/S Layers in sample",1.1802876994542382,1.6457161451870848,1.0834014002788634,1.0317335911347356,0.91695708279423938,1.2267232621945179]
[]
[]
["Comments"]