{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - United Fuel Gas Co 791"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","2HG","3","4","5","6"]
["SAMPLE DEPTH","2264-2276","2323-2330","2323-2330","2330-2342","2342-2350","2350-2364","2364-2374"]
[]
["NON-CLAY FRACTION"]
["Quartz",32.424448984153493,42.396201584403045,36.411056070675428,38.216099638530586,45.582593693615614,46.915457230389919,39.665781106257384]
["K-Feldspar",1.3071778959097795,0.45535674867360165,0.81873610820807452,0,0.73610393981814992,0,0.24531025513779969]
["Plagioclase",3.8441912318237232,6.4492178474784243,4.8628233384466277,8.1447350513627494,7.7600491485456349,8.0720004869227715,6.1672827768874123]
["Organic Carbon (TOC)",0.93899999999999995,0.36,0.375,0.41499999999999998,0.80100000000000005,1.86,0.82599999999999996]
["Apatite",0,0,0,0,0.52262170994890533,0,0]
["Pyrite",2.2535068108271683,0.23505848665251591,0,0.7866100928677785,1.5600006350224689,1.0466749205286869,0.63364724680698803]
["Calcite",0.84637484885512404,0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0,0]
["Siderite",0.37815075915221585,1.2484435412963446,1.4951329377786817,0.79110290518962056,0.32976876552341061,0.33829316212713956,1.0514733912788259]
["Anatase",0.64056952389196253,0.54411786616354307,0.77307665897740951,0.73032216378301495,0.59747374310908019,0.53737602911169047,0.57872171008685158]
["TOTAL",{"$f":"SUM(B9:B18)","v":42.633420054613467},{"$f":"SUM(C9:C18)","v":51.688396074667473},{"$f":"SUM(D9:D18)","v":44.735825114086225},{"$f":"SUM(E9:E18)","v":49.083869851733745},{"$f":"SUM(F9:F18)","v":57.889611635583265},{"$f":"SUM(G9:G18)","v":58.769801829080208},{"$f":"SUM(H9:H18)","v":49.168216486455265}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.282497115328523,4.1336937144158004,7.2921921669223737,2.4239445918993776,3.6149329882367423,3.0038171243527776,3.223494266437303]
["Illite+Mica",41.600282884482283,35.663628873873193,39.889762636434234,39.014889685791523,32.375067341817577,32.471787644276965,37.970046354818997]
["Chlorite",2.0586936770268731,2.5967904904220829,2.3182080005742787,4.5993143543432824,1.4834345192064804,2.4603227672098997,3.8805891687075866]
["Kaolinite",6.4251062685488227,5.9174908466214351,5.7640120819829006,4.8779815162320617,4.6369535151559349,3.29427063508016,5.7576537235808551]
["TOTAL",{"$f":"SUM(B22:B25)","v":57.366579945386505},{"$f":"SUM(C22:C25)","v":48.311603925332506},{"$f":"SUM(D22:D25)","v":55.264174885913789},{"$f":"SUM(E22:E25)","v":50.916130148266248},{"$f":"SUM(F22:F25)","v":42.110388364416742},{"$f":"SUM(G22:G25)","v":41.230198170919806},{"$f":"SUM(H22:H25)","v":50.83178351354475}]
[]
["GRAND TOTAL",{"$f":"B26+B19","v":99.999999999999972},{"$f":"C26+C19","v":99.999999999999972},{"$f":"D26+D19","v":100.00000000000001},{"$f":"E26+E19","v":100},{"$f":"F26+F19","v":100},{"$f":"G26+G19","v":100.00000000000001},{"$f":"H26+H19","v":100.00000000000001}]
[]
["% Expandable Layers in I/S",15.135985798400156,18.919781104400045,15.749574226400114,13.772455958399973,17.794868986399933,13.738367712399963,20.453752174400051]
["% I/S to Illite in <1.0um Fraction",17.945941233484159,11.766073586142419,16.545543520993451,8.0705664027439337,10.64580428382054,9.4189954296154337,9.6476259614603777]
["% Expandable I/S Layers in sample",1.1127262284299837,0.7849114836348986,1.1528122640513667,0.33522789714852619,0.64846680833766501,0.4204966802034063,0.6648169163420663]
[]
[]
["Comments"]