{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Mingo Wymng C & L 814"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","3560-3570","3570-3580","3580-3590","3660-3670","3670-3680","3710-3720"]
[]
["NON-CLAY FRACTION"]
["Quartz",29.539938088558575,26.225543273684835,27.789550345120027,35.156229634405015,35.615460701309907,17.078964166729335]
["K-Feldspar",0.9428833142527373,0.25073629444797318,0.26040733010427775,0.19821380136087732,0.25193516982213182,0.26716960833935693]
["Plagioclase",4.2938457983720175,3.5918644614317352,4.6460684214649781,6.0222428211880423,6.20917399746972,4.2277872468416549]
["Organic Carbon (TOC)",1.55,1.9,3.57,0.30099999999999999,0.36299999999999999,0.22]
["Apatite",0,0,0.13673264373591842,0,0,0]
["Pyrite",1.7319252518915982,2.3664336315486336,2.9776200054666382,0.2349903784889131,0.20050745207914625,0]
["Calcite",0,0,0,0,0,1.6046843747049542]
["Dolomite",0,0,0,0,0,40.356454885605025]
["Siderite",0.3013961536234892,0.19041144393822687,0.19433566214937534,0.48161431664395105,0.3339533617719509,0.16195612850988295]
["Anatase",0.65534263925795522,0.62586522533383848,0.51256920809007078,0.71907106122666398,0.7187424043839773,0.41224675506541586]
["Jarosite",0.92683507580485325,1.5087924481896413,1.722735501084097,0,0,0]
["TOTAL",{"$f":"SUM(B9:B19)","v":39.942166321761214},{"$f":"SUM(C9:C19)","v":36.659646778574874},{"$f":"SUM(D9:D19)","v":41.810019117215383},{"$f":"SUM(E9:E19)","v":43.11336201331347},{"$f":"SUM(F9:F19)","v":43.69277308683683},{"$f":"SUM(G9:G19)","v":64.329263165795624}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",10.22478362062464,14.040818851320196,19.613895914314043,9.341474152910461,6.5000713747552039,2.8353345498872482]
["Illite+Mica",42.005849376390856,43.476309922094508,34.011626969037984,40.195041699624724,44.068993384824026,28.441726129714237]
["Chlorite",3.8042847073134625,1.5720558718833,1.031442894587639,4.6841395771486276,3.3623661659612121,3.149451476219514]
["Kaolinite",4.022915973909817,4.2511685761271147,3.5330151048449383,2.6659825570027329,2.3757959876227241,1.2442246783833566]
["TOTAL",{"$f":"SUM(B23:B26)","v":60.057833678238779},{"$f":"SUM(C23:C26)","v":63.340353221425119},{"$f":"SUM(D23:D26)","v":58.189980882784603},{"$f":"SUM(E23:E26)","v":56.886637986686551},{"$f":"SUM(F23:F26)","v":56.307226913163163},{"$f":"SUM(G23:G26)","v":35.670736834204348}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":99.999999999999986},{"$f":"E27+E20","v":100.00000000000003},{"$f":"F27+F20","v":100},{"$f":"G27+G20","v":99.999999999999972}]
[]
["% Expandable Layers in I/S",12.74980857840012,11.352190492399927,11.590808214399999,14.420132632399941,14.181514910399983,12.783896824400017]
["% I/S to Illite in <1.0um Fraction",23.169340250706188,26.171471971516027,37.600117251145385,22.416317851774696,14.502701706691527,9.8436454258729835]
["% Expandable I/S Layers in sample",1.3241648950586598,1.6248119293523628,2.3575744672821517,1.3511198333694892,0.92516694721594417,0.36326542742448636]
[]
["% Fe in Dolomite/Ankerite",null,null,null,null,null,44.111551200000577]
[]
["Comments"]