{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Mary L S Perkins 7 1166"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2109-2120","2120-2130","2264-2274","2274-2284","2284-2294","no depth"]
[]
["NON-CLAY FRACTION"]
["Quartz",29.948277676149463,29.547785961949732,35.048048465996835,34.087064251379005,33.387702845504755,27.90958639753898]
["K-Feldspar",0.86242569722790308,0.89589749112606909,0.2186661204141265,0.1287975858321572,0.53469985589783553,0.33795326436410439]
["Plagioclase",4.0932717821573235,3.5901720859241553,6.3932405088981854,5.2826651417287307,5.4217463648236697,4.0194016736231584]
["Organic Carbon (TOC)",1.67,2.48,5.24,5.45,4.32,3.49]
["Apatite",0,0,0,0,7.7258498913703828E-3,0]
["Pyrite",2.4346930470789432,2.3374978777546067,2.0061116912109553,1.9113827652529223,1.5897325199803536,2.0912514378080367]
["Calcite",0,0,0,0,0.86091129986932446,0]
["Dolomite",0,0,0,0,0.48800635602900594,0]
["Siderite",0.28977231530456327,0.19991517733989536,0.39665339607662115,0.28589281021312307,0.57145037574030266,0.23663253249744606]
["Anatase",0.73879017460257645,0.4875507767782552,0.53209076001159894,0.4243615540282587,0.51568862231867785,0.46613169523453019]
["TOTAL",{"$f":"SUM(B9:B18)","v":40.037230692520772},{"$f":"SUM(C9:C18)","v":39.538819370872709},{"$f":"SUM(D9:D18)","v":49.834810942608328},{"$f":"SUM(E9:E18)","v":47.570164108434199},{"$f":"SUM(F9:F18)","v":47.697664090055291},{"$f":"SUM(G9:G18)","v":38.550957001066251}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",9.1391856959265372,10.106647881138226,5.6996326945193081,8.5397633854557213,9.5392294005668692,8.8367310203539482]
["Illite+Mica",44.931101790943856,46.681949785171319,37.843180578584956,38.424728082435038,37.438619816916457,47.842904143060871]
["Chlorite",2.3564412188082948,1.9461152297375588,2.9842860501704163,2.7036102980640737,2.3026737570970321,2.7577018006742406]
["Kaolinite",3.536040601800539,1.7264677330801732,3.6380897341169995,2.7617341256109622,3.0218129353643444,2.0117060348446931]
["TOTAL",{"$f":"SUM(B22:B25)","v":59.962769307479221},{"$f":"SUM(C22:C25)","v":60.46118062912727},{"$f":"SUM(D22:D25)","v":50.165189057391686},{"$f":"SUM(E22:E25)","v":52.429835891565794},{"$f":"SUM(F22:F25)","v":52.302335909944702},{"$f":"SUM(G22:G25)","v":61.449042998933749}]
[]
["GRAND TOTAL",{"$f":"B26+B19","v":100},{"$f":"C26+C19","v":99.999999999999972},{"$f":"D26+D19","v":100.00000000000001},{"$f":"E26+E19","v":100},{"$f":"F26+F19","v":100},{"$f":"G26+G19","v":100}]
[]
["% Expandable Layers in I/S",13.738367712400077,15.033721060400012,13.431573498400098,11.556719968399989,19.328840056400054,19.80607550039997]
["% I/S to Illite in <1.0um Fraction",19.149632291177255,19.781155255289949,15.216829489148996,20.887966486425839,22.880483738633693,17.379040768400817]
["% Expandable I/S Layers in sample",1.2768991526751319,1.5580447610819823,0.80788344713297033,1.0438038502602562,1.9270718995073788,1.8135007954186793]
[]
[]
["Comments"]