{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Berwind E 923"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","3293-3312","3312-3325","3325-3330","3342-3357","3357-3367"]
[]
["NON-CLAY FRACTION"]
["Quartz",26.908962331210819,24.118266428581517,26.620483233419129,32.93388651702508,35.745491589971323]
["K-Feldspar",0.64500102758416844,0.26927020567759807,0.26724990874292442,0.20540609248982747,0.25865268137978742]
["Plagioclase",4.7758638812070453,4.3856593434382196,4.0298580942413995,5.3154259238695936,5.9652958751838101]
["Organic Carbon (TOC)",0.46600000000000003,1.62,2.4900000000000002,0.216,0.22700000000000001]
["Apatite",0,0,0,0,0]
["Pyrite",0.54712866673745786,2.2682115218230936,2.3359811110341608,0.28173607718292876,0.23191273765512255]
["Marcasite",0,0,0,0,0]
["Calcite",0,0,0,0,0]
["Dolomite",0,0,0,0,0]
["Siderite",1.5191170756909234,0.29956029689056501,0.6660385277833708,1.304619941107193,1.3317167458750461]
["Anatase",0.86342489911040698,0.75818073450987367,0.78045606690316649,0.86384357126064582,0.789340401392012]
["Jarosite",0,0.57393754604810998,0.49282215040808236,0,0]
["TOTAL",{"$f":"SUM(B9:B20)","v":35.725497881540818},{"$f":"SUM(C9:C20)","v":34.293086076968969},{"$f":"SUM(D9:D20)","v":37.682889092532228},{"$f":"SUM(E9:E20)","v":41.120918122935272},{"$f":"SUM(F9:F20)","v":44.5494100314571}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.1671264548653291,9.2295071598181782,10.711372513360679,9.994632910812058,5.6926537108107356]
["Illite+Mica",46.098588763195927,47.955677060735077,41.909807004278001,38.732927854784535,39.485319887535134]
["Chlorite",4.9069694049634327,3.7602365807851674,4.2478094237949167,5.6945285046483178,5.8272769630203261]
["Kaolinite",6.1018174954344957,4.761493121692606,5.4481219660341722,4.45699260681981,4.4453394071767116]
["TOTAL",{"$f":"SUM(B24:B27)","v":64.274502118459196},{"$f":"SUM(C24:C27)","v":65.706913923031024},{"$f":"SUM(D24:D27)","v":62.317110907467772},{"$f":"SUM(E24:E27)","v":58.879081877064721},{"$f":"SUM(F24:F27)","v":55.450589968542907}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":100.00000000000001},{"$f":"C28+C21","v":100},{"$f":"D28+D21","v":100},{"$f":"E28+E21","v":100},{"$f":"F28+F21","v":100}]
[]
["% Expandable Layers in I/S",15.988191948400072,11.28401400040002,14.897368076400085,15.954103702400062,15.885927210400041]
["% I/S to Illite in <1.0um Fraction",15.318798512006875,18.096051808834694,23.447582371470009,25.541754824848965,15.850649296143366]
["% Expandable I/S Layers in sample",1.151258800800159,1.058608335110597,1.6364604546709953,1.5980057917753963,0.90638832634032285]
[]
[]
["Comments"]