{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Courtlnd Co TR-64 1692"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","4HG"]
["SAMPLE DEPTH","1828-1838","1838-1850","1850-1864","1864-1874","1864-1874"]
[]
["NON-CLAY FRACTION"]
["Quartz",38.465503102486821,30.125743861199762,25.06613115962206,36.228354703527017,30.674015126933888]
["K-Feldspar",0.21250556860201916,0.3650413881555446,0.24476465908001099,0.24303178390445629,0.39940797367192465]
["Plagioclase",7.2966686006147254,4.6536911647452079,4.01612444841287,5.4070792264114802,4.1625153091904261]
["Organic Carbon (TOC)",0.36699999999999999,0.499,2.84,2.11,2.19]
["Apatite",0,5.5646057000561633E-2,0,0,0]
["Pyrite",0.27583198046644425,0.81022965091349652,2.2761087534937383,1.7318687885064334,1.2163705512391829]
["Marcasite",0,0,1.0683609014496172,0.66299822630898586,0.66353970185107503]
["Calcite",0,0,0,0.39860536713767736,0]
["Dolomite",0,0,0,0,0]
["Siderite",0.48208173091990431,0.35091025036712847,0.11807235145410673,0.22189560546351628,0.28545781760846972]
["Gypsum",0,0.4085976197739345,0.32388222216760448,0.67039060248633464,0]
["Anatase",0.79950490749785519,0.84200441141071902,0.64814022669232219,0.46912349747727045,0.75535175850693814]
["TOTAL",{"$f":"SUM(B9:B20)","v":47.899095890587759},{"$f":"SUM(C9:C20)","v":38.110864403566353},{"$f":"SUM(D9:D20)","v":36.60158472237233},{"$f":"SUM(E9:E20)","v":48.143347801223172},{"$f":"SUM(F9:F20)","v":40.346658239001897}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",5.2290527290489566,8.7896527676020177,11.34910863952606,11.439004903838299,9.8787663674660564]
["Illite+Mica",36.381022700553196,40.586403769161159,43.342540476475378,31.358698061374664,40.388078200582044]
["Chlorite",4.5328798481640336,5.8008300898123135,3.3052231940956931,3.4215937738244104,3.8464416524348697]
["Kaolinite",5.9579488316460463,6.7122489698581491,5.4015429675305615,5.6373554597394504,5.5400555405151168]
["TOTAL",{"$f":"SUM(B24:B27)","v":52.100904109412241},{"$f":"SUM(C24:C27)","v":61.88913559643364},{"$f":"SUM(D24:D27)","v":63.398415277627691},{"$f":"SUM(E24:E27)","v":51.856652198776828},{"$f":"SUM(F24:F27)","v":59.653341760998089}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":100},{"$f":"C28+C21","v":100},{"$f":"D28+D21","v":100.00000000000003},{"$f":"E28+E21","v":100},{"$f":"F28+F21","v":99.999999999999986}]
[]
["% Expandable Layers in I/S",16.942662836400018,12.954338054400068,10.874955048400011,11.624896460400009,12.579367348399956]
["% I/S to Illite in <1.0um Fraction",15.037728400383028,23.754142610360269,24.866192376729749,31.36760278462048,23.247041189014112]
["% Expandable I/S Layers in sample",0.88920415266060293,1.1443516480468507,1.2702866024521831,1.3584354644716337,1.2705104905978337]
[]
[]
["Comments"]