{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea Project - Rosin Coal Land 2 1785"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3"]
["SAMPLE DEPTH","2005-2014","2014-2021","2021-2032"]
[]
["NON-CLAY FRACTION"]
["Quartz",27.667963566718758,30.638890502431188,33.311922599097741]
["K-Feldspar",0,0,0]
["Plagioclase",3.4605568526696078,3.3675741318915318,7.2090261101208579]
["Organic Carbon (TOC)",1.31,2.96,2.0499999999999998]
["Apatite",0.5776399912902227,0.4886127941744281,7.9520356953138652E-2]
["Pyrite",1.3021822827689316,2.2029057020510567,1.2914154249233945]
["Marcasite",0,0.57947263394457083,0]
["Calcite",0,0,0.59823883499689834]
["Dolomite",0,0,0]
["Siderite",0,0,0.74744267625302097]
["Gypsum",0.39969845887188238,0.36085481769022737,0.27257473446626362]
["TOTAL",{"$f":"SUM(B9:B19)","v":34.718041152319401},{"$f":"SUM(C9:C19)","v":40.598310582182997},{"$f":"SUM(D9:D19)","v":45.560140736811313}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",8.1123650030798888,8.9032107948938801,6.8827066442085787]
["Illite+Mica",43.504312992487534,40.017077662142462,35.12373379214516]
["Chlorite",9.1812713118288922,5.5281597017527444,7.640659094114441]
["Kaolinite",4.4840095402842719,4.9532412590279229,4.7927597327204854]
["TOTAL",{"$f":"SUM(B23:B26)","v":65.281958847680585},{"$f":"SUM(C23:C26)","v":59.401689417817011},{"$f":"SUM(D23:D26)","v":54.439859263188666}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":99.999999999999986},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":99.999999999999972}]
[]
["% Expandable Layers in I/S",9.9204841604000649,9.5796017003999623,10.568160834400146]
["% I/S to Illite in <1.0um Fraction",19.821097697076439,21.873309925100099,21.786531594908432]
["% Expandable I/S Layers in sample",0.81546852281323212,0.8789078036869814,0.74259878297080928]
[]
[]
["Comments"]