{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea - Horse CR L & M 47 519"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","2220-2227","2231-2234","2234-2239","2239-2246","no depth-2227"]
[]
["NON-CLAY FRACTION"]
["Quartz",25.008497056774104,28.329740081878139,23.305653969441245,24.058394539708839,25.853353790841883]
["K-Feldspar",0.77098086201089211,1.3925145882006087,1.5843604785918459,0.74287718545832249,0.47005933560202584]
["Plagioclase",4.8798639297194306,4.1377293014480747,4.0503719790925876,3.8310011232167995,4.4488618565422602]
["Organic Carbon (TOC)",0.53600000000000003,0.44600000000000001,0.40799999999999997,0.379,2.42]
["Apatite",0,0,0,0,0]
["Pyrite",0.3100668419443966,0,0,0,1.6017122914477679]
["Marcasite",0,0,0,0,0]
["Calcite",0,0,0,0,0]
["Dolomite",0,0,0,0,0]
["Siderite",1.592793764889713,0.53250782694696697,0.65595019771650076,0.6611706594383564,0.35867678422742877]
["Anatase",0.81311592881839789,0.77133556246053725,0.86281324011339222,0.78162383974756344,0.52477690072950145]
["TOTAL",{"$f":"SUM(B9:B19)","v":33.911318384156935},{"$f":"SUM(C9:C19)","v":35.609827360934325},{"$f":"SUM(D9:D19)","v":30.867149864955575},{"$f":"SUM(E9:E19)","v":30.454067347569882},{"$f":"SUM(F9:F19)","v":35.677440959390864}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.4327219828160587,6.8652646095190129,6.7165746895264391,5.2025293989583004,13.75375805990573]
["Illite+Mica",48.148886775212091,47.760125998435313,52.527200339485219,54.36545813971663,44.8895383551056]
["Chlorite",4.0370469537915197,3.4996802097171691,3.8958020836328928,3.1476787433918876,2.079360657813119]
["Kaolinite",6.4700259040233865,6.2651018213941772,5.9932730223998618,6.8302663703633115,3.5999019677846942]
["TOTAL",{"$f":"SUM(B23:B26)","v":66.088681615843058},{"$f":"SUM(C23:C26)","v":64.390172639065682},{"$f":"SUM(D23:D26)","v":69.132850135044407},{"$f":"SUM(E23:E26)","v":69.545932652430125},{"$f":"SUM(F23:F26)","v":64.322559040609136}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":99.999999999999986},{"$f":"E27+E20","v":100},{"$f":"F27+F20","v":100}]
[]
["% Expandable Layers in I/S",16.738133360399956,17.760780740400037,20.72645814240002,18.374369168399994,9.6477781923999828]
["% I/S to Illite in <1.0um Fraction",15.265131589740086,13.88739444870877,12.249832993669454,9.1537266798918484,24.47179955970952]
["% Expandable I/S Layers in sample",1.2508032230671562,1.2247871452126007,1.3978111109604501,0.95956872332052445,1.3598402036678001]
[]
[]
["Comments"]