{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea - TCO Min TR 1 1319 "]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2300-2314","2314-2328","2328-2336","2382-2394","2394-2405","2405-2415"]
[]
["NON-CLAY FRACTION"]
["Quartz",34.108527265607137,32.134517533222848,32.394671486467978,48.342603535304988,47.885528513478917,46.136306590030784]
["K-Feldspar",0.78892533259407149,0.26774513731543004,0.32349915725209649,0.45947229632914399,0.51446539835106053,0.37406258157041766]
["Plagioclase",5.0110835494315484,5.1696003335505578,4.5547303676039199,8.3437957467957435,9.5817851480776692,7.3603340641686508]
["Organic Carbon (TOC)",0.46200000000000002,2.42,1.66,0.85299999999999998,1.24,1.07]
["Apatite",0,0,0,0.20571807203144821,0,0]
["Pyrite",0.7523624869991874,1.4081127967993632,1.2241262718428567,0.7888381098909546,1.0333629153463346,1.003790509930292]
["Marcasite",0,0.32466945986037021,0,0,0,0]
["Calcite",0,0.48490469515546974,0,0,0,0]
["Dolomite",0,0,0,1.7820091049494995,1.2391633553823787,0.90717577501072744]
["Siderite",1.8172634397755461,0.20416381943568654,0.99398826193741907,0.44014577553409817,0.30356512846759964,0.22649942424828196]
["Gypsum",0,0,0.42108847962617096,0.25112639816776294,0.2515538513174827,0.27608318458562842]
["Anatase",0.54700867229726491,0.53908409919118694,0.50110656787926955,0.35218806896396049,0.4447283437687175,0.44813720314448929]
["TOTAL",{"$f":"SUM(B9:B20)","v":43.487170746704756},{"$f":"SUM(C9:C20)","v":42.952797874530908},{"$f":"SUM(D9:D20)","v":42.073210592609705},{"$f":"SUM(E9:E20)","v":61.818897107967601},{"$f":"SUM(F9:F20)","v":62.494152654190167},{"$f":"SUM(G9:G20)","v":57.802389332689273}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",7.8250713826538396,14.072288922506177,10.427055954438787,7.2349103610494119,6.4380552663193367,6.314560815826411]
["Illite+Mica",39.585678790789558,39.163455746321681,41.180217189559997,24.698314079583458,25.251992446583195,29.234404187728124]
["Chlorite",2.5438985103878409,2.1513989224848777,2.3573435338881921,2.0761651030675567,2.1899142213584288,2.4478149056623457]
["Kaolinite",6.5581805694639943,1.6600585341563481,3.9621727295033069,4.1717133483319815,3.625885411548877,4.2008307580938551]
["TOTAL",{"$f":"SUM(B24:B27)","v":56.51282925329523},{"$f":"SUM(C24:C27)","v":57.047202125469084},{"$f":"SUM(D24:D27)","v":57.926789407390281},{"$f":"SUM(E24:E27)","v":38.181102892032413},{"$f":"SUM(F24:F27)","v":37.50584734580984},{"$f":"SUM(G24:G27)","v":42.197610667310741}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":99.999999999999986},{"$f":"C28+C21","v":100},{"$f":"D28+D21","v":99.999999999999986},{"$f":"E28+E21","v":100.00000000000001},{"$f":"F28+F21","v":100},{"$f":"G28+G21","v":100.00000000000001}]
[]
["% Expandable Layers in I/S",15.272338782399856,10.499984342400012,12.988426300400079,12.374837872400008,13.261132268400047,13.533838236400015]
["% I/S to Illite in <1.0um Fraction",18.25412222635471,29.440688521416746,21.783865331039021,25.12603953196491,23.15251474590081,20.126511669433732]
["% Expandable I/S Layers in sample",1.2006182679213118,1.5142325614679653,1.3771715252631278,0.90301111218023167,0.86447855850476107,0.86384559400894301]
[]
["% Fe in Dolomite/Ankerite",null,null,null,68.260060099999464,72.492272999999841,70.749597099998937]
[]
["Comments"]