{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":39,"n_cols":7,"rows_kept":39,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea - Ray Lovejoy 1383"]
["JOB #","15-0601"]
["SAMPLE ID","1","3","2","4","5","6"]
["SAMPLE DEPTH","2482-2490","2540-2547","2502-2575","2586-2596","2596-2605","no depth"]
[]
["NON-CLAY FRACTION"]
["Quartz",34.475791243765713,30.66667594251545,38.126670415201765,35.009167896957678,38.253483842573964,39.810568425884227]
["K-Feldspar",0.47628538671652326,0.5491296631339817,0.33226336512564919,0.3026653575989004,0.28978866683671217,0.30343967955016704]
["Plagioclase",5.8730297883870115,5.0077707055208887,5.5816175533076295,6.0378030462160144,6.9872803593644299,6.1917560705455079]
["Organic Carbon (TOC)",0.34200000000000003,2.04,0.373,0.29299999999999998,0.34499999999999997,0.28399999999999997]
["Apatite",0,0,0,0,0,0]
["Pyrite",0.26617300962173984,0.89367281570788271,0.31821056096958295,0.53296975992607754,0.46929289975468069,1.1034325100181421]
["Marcasite",0,0,0,0,0,0]
["Calcite",0,0,0.50446785362214175,0,0,0]
["Dolomite",0,0,0,2.2137900047968504,0.93177503427268404,0.70590810770834911]
["Siderite",0.94626572620802152,0.46008895996962751,0.68081197949375072,0.84363182816202786,0.31463517058536628,0.2958131745982619]
["Gypsum",0,0.85788955393715527,0,0.24217873747160548,0.74346342476569927,0.55163734416647003]
["Anatase ",0.63207453030783578,0.48085751318980169,0.68747593677320107,0.58873153704674808,0.5921054206704125,0.53321203056239519]
["Jarosite ",0,1.4956393234299363,0,0,0,0]
["TOTAL",{"$f":"SUM(B9:B21)","v":43.011619685006842},{"$f":"SUM(C9:C21)","v":42.451724477404717},{"$f":"SUM(D9:D21)","v":46.60451766449372},{"$f":"SUM(E9:E21)","v":46.063938168175888},{"$f":"SUM(F9:F21)","v":48.926824818823945},{"$f":"SUM(G9:G21)","v":49.779767343033519}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.2198700672262923,12.248536523197849,5.6553272807942063,4.2502881367377485,6.4677910926827735,9.5439910993760559]
["Illite+Mica",40.470539429345138,40.962453236588367,37.849564641222692,41.393672953355605,36.21404891559051,34.145666248471336]
["Chlorite",3.3688715576819126,1.6860194154822974,3.7122465021545095,4.135802661799584,3.7383697566206457,2.9189829516597383]
["Kaolinite",6.9290992607398163,2.6512663473267581,6.1783439113348804,4.1562980799311449,4.6529654162821208,3.6115923574593523]
["TOTAL",{"$f":"SUM(B25:B28)","v":56.988380314993165},{"$f":"SUM(C25:C28)","v":57.548275522595276},{"$f":"SUM(D25:D28)","v":53.39548233550628},{"$f":"SUM(E25:E28)","v":53.936061831824091},{"$f":"SUM(F25:F28)","v":51.073175181176047},{"$f":"SUM(G25:G28)","v":50.220232656966481}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":100},{"$f":"C29+C22","v":100},{"$f":"D29+D22","v":100},{"$f":"E29+E22","v":99.999999999999972},{"$f":"F29+F22","v":100},{"$f":"G29+G22","v":100}]
[]
["% Expandable Layers in I/S",18.783428120400004,8.7955720424000674,13.874720696400004,14.249691402400003,11.181749262400103,10.534072588399908]
["% I/S to Illite in <1.0um Fraction",14.607944150558188,24.103392696986077,15.686202846853378,10.951364444013389,18.85245235606649,25.522360201320215]
["% Expandable I/S Layers in sample",1.1723141376103536,1.0997640404629965,0.78759860748342259,0.60743272107068347,0.72571590266382602,1.0082343357522365]
[]
["% Fe in Dolomite/Ankerite",null,null,null,64.276800899999216]
[]
["Comments"]