{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["TOC RE6 Data","Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TOC RE6 Data","index":0,"n_rows":35,"n_cols":15,"rows_kept":35,"cut":false,"hidden":false,"merged":[[10,1,11,3],[32,0,32,5],[31,0,31,5],[0,0,0,15],[18,0,23,0]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / RE6"]
[]
["Job Number:","15-0601"]
["Well Name:","Berea Project - D E MCCORMICK #1469"]
["Formation:","Berea / Cleaveland / Sunberry"]
["Sample Type:","cuttings"]
["Sample Size:","20/40 mesh"]
["Instrumentation:","LECO C230 & Rock-Eval 6"]
[]
[]
[null,"Total Organic Carbon (TOC) Reference Standard Results"]
[]
[null,"Date","TOC Result","% Recovery"]
[null,"2015-06-12",5.85,{"$f":"(C14/5.85)*100","v":100}]
[]
[]
[]
["DATE","Depth Range","Ave. Depth","SAMPLE ID","S1 (mg/g)","S2 (mg/g)","S3 (mg/g)","Tmax (°C)","S1+S2","Calc. %Ro-Tmax","TOC (% wt)","HI","OI","PI","NOC"]
["2015-06-12","2130-2140",2635,1,null,null,null,null,null,null,0.247]
[null,"2140-2150",2145,2,null,null,null,null,null,null,0.219]
[null,"2330-2340",2335,3,null,null,null,null,null,null,0.46600000000000003]
[null,"2340-2350",2345,4,null,null,null,null,null,null,0.50700000000000001]
[null,"2350-2360",2355,5,null,null,null,null,null,null,0.435]
[null,"2360-2370",2365,6,null,null,null,null,null,null,0.39900000000000002]
[]
[]
["RE6 analysis not performed on samples with TOC values < 1.50%"]
["S1 = Volatile Total Petroleum Hydrocarbons (mg/g)"]
["S2 = Kerogen yield (mg/g)"]
["HI = Hydrogen Index"]
["PI = Production Index"]
["Calc. %Ro-Tmax = Calculated%VRo = 0.0180 x Tmax - 7.16 (Jarvie et al., 2001)"]
["NOC = Normalized Oil Content = (S1/TOC) x 100 (Jarvie and Baker, 1984)"]
[]
["LECO B"]

{"sheet":"Sheet1","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":true,"merged":[[0,1,0,2],[5,1,5,2],[10,1,10,2],[15,1,15,2]]}
[null,"HI 700 LINE"]
[null,"y","x"]
[null,0,0]
[null,300,42.85]
[]
[null,"HI 350 LINE"]
[null,"y","x"]
[null,0,0]
[null,280,80]
[]
[null,"HI 200 LINE"]
[null,"y","x"]
[null,0,0]
[null,160,80]
[]
[null,"HI 50 LINE"]
[null,"y","x"]
[null,0,0]
[null,40,80]