{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT","Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Fee 1648 "]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2350-2360","2360-2370","2370-2380","2450-2460","2460-2470","2470-2480"]
[]
["NON-CLAY FRACTION"]
["Quartz",34.988675906317212,34.69345670970759,30.045973544891503,50.573309877451635,41.888410219629769,42.452282516147193]
["K-Feldspar",0.48316781050435315,0.18328064676297873,0.29657580281813006,0.37966530369400892,0.36164520956933871,0.12983658661284705]
["Plagioclase",5.6503107670224884,5.3429572602860178,4.1814077957559315,11.060043434716587,10.449116390124209,9.2773539317684666]
["Organic Carbon (TOC)",0.64300000000000002,0.81200000000000006,2.95,1.88,1.5,1.43]
["Apatite",0.23277400545616392,0,0,0,0,0]
["Pyrite",2.0701646168412804,2.0744319990964613,6.025013122496758,1.5901074383664662,1.9680841627070191,2.2292351459076962]
["Marcasite",0,0,1.1934646137375455,0,0,0]
["Calcite",0.75081539893144511,0.51016033053050114,0.51730775851607547,0,0,0.38227726392491529]
["Dolomite",0,0,0,0.63277550615668154,0.77398476303596386,0.45276092697446724]
["Siderite",0.57275536873764066,0.72991366431673721,0.22126319977417458,0.21524490786374789,0.21846805666840105,0.20572022764141398]
["Gypsum",0.57139934076584331,0.42500188014219481,0.56280845067663909,0.35507880541074355,0.36164520956933871,0.26977263227641857]
["Anatase ",0.57866742109625113,0.58090074745967757,0.37309547744728522,0.40330805924412144,0.38153007130411609,0.52424028828423097]
["Jarosite",0,0.73962727399243389,0.4544093667354196,0,0,0]
["TOTAL",{"$f":"SUM(B9:B21)","v":46.541730635672678},{"$f":"SUM(C9:C21)","v":46.091730512294603},{"$f":"SUM(D9:D21)","v":46.821319132849474},{"$f":"SUM(E9:E21)","v":67.089533332903997},{"$f":"SUM(F9:F21)","v":57.902884082608153},{"$f":"SUM(G9:G21)","v":57.35347951953765}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.8045964577350571,12.07328556010715,12.469698910303899,5.483887471251645,6.6261918747019504,5.9724609739950516]
["Illite+Mica",39.652183642357613,34.84366279769182,36.173098058892762,20.467812067903012,29.045745496874503,30.634785199972661]
["Chlorite",2.0826406285455445,2.0604465042517144,2.5144806939226667,2.5622475384587982,3.2687667174470523,2.866682818208353]
["Kaolinite",4.9188486356891028,4.9308746256547238,2.0214032040312051,4.3965195894825406,3.1564118283683484,3.1725914882863022]
["TOTAL",{"$f":"SUM(B25:B28)","v":53.458269364327322},{"$f":"SUM(C25:C28)","v":53.908269487705411},{"$f":"SUM(D25:D28)","v":53.178680867150526},{"$f":"SUM(E25:E28)","v":32.910466667095996},{"$f":"SUM(F25:F28)","v":42.097115917391854},{"$f":"SUM(G25:G28)","v":42.646520480462364}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":100},{"$f":"C29+C22","v":100.00000000000001},{"$f":"D29+D22","v":100},{"$f":"E29+E22","v":100},{"$f":"F29+F22","v":100},{"$f":"G29+G22","v":100.00000000000001}]
[]
["% Expandable Layers in I/S",15.306427028400094,12.443014364400142,9.8182194224000341,13.67019122040017,10.29545486639995,10.77269031039998]
["% I/S to Illite in <1.0um Fraction",16.763336450520761,28.850080371040292,28.337288195991821,25.945299776124379,22.188667534878249,19.719934050233782]
["% Expandable I/S Layers in sample",1.0482810384575962,1.5145790382900963,1.2615171564412802,0.76402150798172375,0.69258537443756363,0.65272874570151684]
[]
["Comments"]