{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Dingess Rum Co 853"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","3485-3489","3528-3532","3532-3536","3536-3541","3541-3553"]
[]
["NON-CLAY FRACTION"]
["Quartz",29.940299617209622,32.998462644113587,36.05103256831115,31.443349679429915,32.729733876838708]
["K-Feldspar",0.84755337040182499,1.0523851635262893,0.11373884897231476,0.42187990174304202,0.19791835135145114]
["Plagioclase",4.3942248760947242,5.9025513381718397,6.2019577022583592,5.2451067649289591,5.5316865139795715]
["Organic Carbon (TOC)",2.8,0.42499999999999999,0.33300000000000002,0.4,0.45500000000000002]
["Apatite",0,0,0,0,0]
["Pyrite",2.5620714462649614,0.52152153095632314,0.39170125830569152,0.23100287235624056,0.69094077809901511]
["Marcasite",0.70579236819990421,0,0,0,0]
["Calcite",0,0,0,0,0]
["Dolomite",0,0,0,0,0]
["Siderite",0.27433900834604474,2.0450789998220227,0.84124257449471629,1.3288339594209118,0.81011084831008662]
["Anatase",0.75254125080110401,0.70633273912504013,0.72741423146503925,0.81935908569331184,0.84016491172457131]
["TOTAL",{"$f":"SUM(B9:B19)","v":42.276821937318175},{"$f":"SUM(C9:C19)","v":43.651332415715096},{"$f":"SUM(D9:D19)","v":44.660087183807278},{"$f":"SUM(E9:E19)","v":39.889532263572384},{"$f":"SUM(F9:F19)","v":41.255555280303405}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.6431934078239125,4.7276934333548608,5.7778448867423275,6.9027207305809704,6.6944440382042183]
["Illite+Mica",41.106517215110102,43.870668453990788,41.173026795585876,43.973639003484891,43.024958542574318]
["Chlorite",5.2459165146226416,3.5339121554993436,5.0773905656500045,5.735470550143333,4.7709993470493606]
["Kaolinite",4.7275509251251551,4.2163935414399072,3.3116505682145267,3.4986374522184236,4.2540427918687183]
["TOTAL",{"$f":"SUM(B23:B26)","v":57.723178062681818},{"$f":"SUM(C23:C26)","v":56.348667584284897},{"$f":"SUM(D23:D26)","v":55.339912816192736},{"$f":"SUM(E23:E26)","v":60.110467736427616},{"$f":"SUM(F23:F26)","v":58.744444719696617}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":100.00000000000001},{"$f":"E27+E20","v":100},{"$f":"F27+F20","v":100.00000000000003}]
[]
["% Expandable Layers in I/S",17.147192312399966,19.533369532400002,16.397250900400081,18.681163382400086,15.340515274399991]
["% I/S to Illite in <1.0um Fraction",18.303407796227887,11.477965795225565,15.063105222075961,17.073513461824202,16.139216491926369]
["% Expandable I/S Layers in sample",1.1719353388109499,0.9274193609803808,0.95057313124211262,1.294687286657261,1.0316562461367997]
[]
[]
["Comments"]