{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Dingess Rum CL 926"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","2860-2870","2870-2880","2880-2890","2900-2910","2920-2930","2950-2960"]
[]
["NON-CLAY FRACTION"]
["Quartz",26.00267935362913,26.175631078681015,28.842598951816935,29.130466842218564,30.155168809865447,32.859914599740321]
["K-Feldspar",0.81557793922831112,0.66590468490921173,0.25642541622522314,0.25477444736420063,0.21288007838716241,0.2681738151895513]
["Plagioclase",4.2085903964750369,3.597706317444278,4.5759007999536703,4.5135482961814057,5.0728123058368366,5.6641110138236757]
["Organic Carbon (TOC)",2.5099999999999998,3.03,2.88,2.92,0.313,0.39200000000000002]
["Apatite",0,0.25873359160000464,0,0,0,0]
["Pyrite",3.4405093515852223,3.3209110806300837,2.86062785484107,2.0697120397027375,0.24055292628640107,0.8486440392384651]
["Marcasite",1.1247495356640944,0.55173191196727311,0.70442895057252097,0.48461794766670241,0,0]
["Calcite",0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0]
["Siderite",0.45293492296262983,0.26242097150121324,0.28857095464391946,0.20492992727220463,1.2505850358608275,0.84577699655855498]
["Anatase",0.75016638621307052,0.56198620104421804,0.5818189576812447,0.60904555727351739,0.87147956204388299,0.68833986235698186]
["TOTAL",{"$f":"SUM(B9:B19)","v":39.305207885757483},{"$f":"SUM(C9:C19)","v":38.425025837777298},{"$f":"SUM(D9:D19)","v":40.990371885734582},{"$f":"SUM(E9:E19)","v":40.187095057679329},{"$f":"SUM(F9:F19)","v":38.116478718280554},{"$f":"SUM(G9:G19)","v":41.566960326907555}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.7446614616461256,9.001275532923696,11.497099118055221,11.351268601301316,7.6119675231354051,6.8305596790700882]
["Illite+Mica",46.201397066622704,44.218452125975915,40.906058787346616,40.594926861613736,46.626160164866064,41.412591621761493]
["Chlorite",4.0904656314871648,4.3287895478091771,2.7259937847468469,3.7440737235503345,3.7666038436192233,5.1325097993680338]
["Kaolinite",3.6582679544864947,4.0264569555139076,3.8804764241167384,4.1226357558552786,3.8787897500987643,5.0573785728928131]
["TOTAL",{"$f":"SUM(B23:B26)","v":60.694792114242489},{"$f":"SUM(C23:C26)","v":61.574974162222702},{"$f":"SUM(D23:D26)","v":59.009628114265425},{"$f":"SUM(E23:E26)","v":59.812904942320664},{"$f":"SUM(F23:F26)","v":61.883521281719453},{"$f":"SUM(G23:G26)","v":58.433039673092438}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":99.999999999999972},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":100},{"$f":"E27+E20","v":100},{"$f":"F27+F20","v":100},{"$f":"G27+G20","v":100}]
[]
["% Expandable Layers in I/S",11.999867166400009,14.454220878399951,11.386278738400051,12.204396642399956,12.71572033240011,12.920249808400058]
["% I/S to Illite in <1.0um Fraction",15.491977690296261,21.183904942688844,24.527378060213657,25.997160285098062,16.215785833341553,16.190749385740183]
["% Expandable I/S Layers in sample",0.83018813849718798,1.3417183122637553,1.3479116066844128,1.4270229131098253,0.97095559304124057,0.88599848792035263]
[]
[]
["Comments"]