{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Williamson M&M #2 719"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","2654-2676","2676-2686","2686-2700","2854-2864","2864-2874"]
[]
["NON-CLAY FRACTION"]
["Quartz",33.066021519895841,36.170129150596324,35.949231047042595,33.562286469332903,33.533580833578647]
["K-Feldspar",0.69188722997788188,0.27258836367393513,0.73323225759365118,0.23465575310756767,0.25154155994467631]
["Plagioclase",5.6584770538099471,5.6577050047547361,6.0211358722860444,3.0941152201945799,4.9566953983664108]
["Organic Carbon (TOC)",0.36099999999999999,0.39700000000000002,0.40899999999999997,0.30599999999999999,3.62]
["Apatite",0,0,0.40336350058443965,0,2.7007015666674884E-2]
["Pyrite",0.40305146337064435,0.41790355864957207,0.72473974927133256,0,1.2214604517823944]
["Marcasite",0,0,0,0,0]
["Calcite",0,0,0,0,0]
["Dolomite",0,0,0,0,0]
["Siderite",2.8052016111176719,1.8106453225186216,2.5067602414372629,2.1628991394525938,0.55999048776240623]
["Anatase",0.55496941954588141,0.63622105926041539,0.58027581239071357,0.69722755445473816,0.54809276773614923]
["TOTAL",{"$f":"SUM(B9:B19)","v":43.540608297717867},{"$f":"SUM(C9:C19)","v":45.362192459453603},{"$f":"SUM(D9:D19)","v":47.327738480606037},{"$f":"SUM(E9:E19)","v":40.057184136542382},{"$f":"SUM(F9:F19)","v":44.718368514837358}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.4058622976341804,6.7018925804941603,8.0147781813570962,6.0551427444433426,8.3276691464579429]
["Illite+Mica",40.766955531832004,37.986912537543262,35.102338431748841,43.223525536130886,39.359429574779746]
["Chlorite",3.3004786263239119,2.9299510360631063,2.4252139287659054,2.572012367948894,2.585486267817021]
["Kaolinite",5.9860952464920452,7.0190513864458586,7.1299309775221067,8.0921352149344834,5.0090464961079411]
["TOTAL",{"$f":"SUM(B23:B26)","v":56.459391702282133},{"$f":"SUM(C23:C26)","v":54.63780754054639},{"$f":"SUM(D23:D26)","v":52.672261519393949},{"$f":"SUM(E23:E26)","v":59.942815863457611},{"$f":"SUM(F23:F26)","v":55.281631485162649}]
[]
["GRAND TOTAL",{"$f":"B27+B20","v":100},{"$f":"C27+C20","v":100},{"$f":"D27+D20","v":99.999999999999986},{"$f":"E27+E20","v":100},{"$f":"F27+F20","v":100}]
[]
["% Expandable Layers in I/S",17.010839328400152,15.442780012400135,14.863279830399961,17.590339510399986,13.874720696400004]
["% I/S to Illite in <1.0um Fraction",15.058888781729442,16.988156112389294,20.781418593709002,14.844498852867051,20.648290271686765]
["% Expandable I/S Layers in sample",1.0936389797660682,1.0390836901228679,1.1961511671546086,1.0683894382680355,1.1988387991194414]
[]
[]
["Comments"]