{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Huntington Realty 879"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","2330-2340","2430-2440","2450-2460","2460-2470","2540-2550"]
[]
["NON-CLAY FRACTION"]
["Quartz",31.076850506762632,34.371546997544399,31.642504299066381,31.170305558868204,38.477952478238166]
["K-Feldspar",0.7107707480112293,0.31966532808473236,0.40025023913204033,0.48566038067582362,0.28442811418559599]
["Plagioclase",4.4971038207073981,5.0906888470117835,5.1699315590132358,5.0421180646980144,4.4328572124369785]
["Organic Carbon (TOC)",0.61299999999999999,0.80300000000000005,0.39700000000000002,0.54400000000000004,3.6]
["Apatite",0,0,0,0,0]
["Pyrite",0.67716418399227429,0.66748730455087446,0.35085610550118235,0.30133333554444675,0.45755171219091145]
["Calcite",0,0.33023134307849716,0,0.37960005961122772,0]
["Dolomite",0,0,0,0,0]
["Siderite",0.9399481038187717,1.327879748431916,1.3932880828041976,1.3296285058491593,1.2847694205176527]
["Anatase",0.80469934818837385,0.73172218006847078,0.66598968442962747,0.7646836702007026,0.63265086842527174]
["TOTAL",{"$f":"SUM(B9:B18)","v":39.31953671148068},{"$f":"SUM(C9:C18)","v":43.642221748770673},{"$f":"SUM(D9:D18)","v":40.01981996994666},{"$f":"SUM(E9:E18)","v":40.017329575447576},{"$f":"SUM(F9:F18)","v":49.170209805994581}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",8.050568110065587,8.5204390382941479,8.1344424185569686,8.5295789080737965,8.7919106361988089]
["Illite+Mica",42.678769600001502,36.144614297223235,40.465759750002121,39.691556414210339,32.512307182591357]
["Chlorite",3.8757443686959623,4.2408887289782138,3.6689840626050949,4.0123221465944523,2.9048614758589446]
["Kaolinite",6.0753812097562667,7.4518361867337326,7.7109937988891515,7.7492129556738369,6.6207108993563075]
["TOTAL",{"$f":"SUM(B22:B25)","v":60.680463288519313},{"$f":"SUM(C22:C25)","v":56.357778251229334},{"$f":"SUM(D22:D25)","v":59.98018003005334},{"$f":"SUM(E22:E25)","v":59.982670424552424},{"$f":"SUM(F22:F25)","v":50.829790194005412}]
[]
["GRAND TOTAL",{"$f":"B26+B19","v":100},{"$f":"C26+C19","v":100},{"$f":"D26+D19","v":100},{"$f":"E26+E19","v":100},{"$f":"F26+F19","v":100}]
[]
["% Expandable Layers in I/S",15.613221242400073,18.374369168399994,17.794868986399933,17.283545296399893,16.601780376400029]
["% I/S to Illite in <1.0um Fraction",18.461317056286806,22.377564330737037,18.906295881220608,20.303421010765508,25.093597466497219]
["% Expandable I/S Layers in sample",1.2647056559657164,1.578250273359715,1.453282904286372,1.4822772222581906,1.5141220899492538]
[]
[]
["Comments"]