{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":41,"n_cols":10,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Twist About Prospect - Lewis HRS PI-1"]
["JOB #","15-0202"]
["SAMPLE ID","1","2","3","4","5","6","7","8","9"]
["SAMPLE DEPTH","2045.50","2049.60","2051.20","2056.30","2070.20","2077.60","2084.80","2089.60","2096.60"]
[]
["NON-CLAY FRACTION"]
["Quartz",3.2480355959207299,25.926912784772288,84.711686819081535,81.324780112074095,77.513226422335151,66.492847994398304,26.245357277688147,69.61124868741031,76.667623895219748]
["K-Feldspar",0,0.23639551394137098,0.85885906236766285,0.93042669836885361,1.4917385981902989,1.2049446093425087,0.55183759766593299,0.55054865015497134,1.8579238662871722]
["Plagioclase",7.0758046582088105E-2,0.81971289497494715,1.221654907356317,2.43698733675317,2.5343240464133823,2.5581125479488951,0,2.0882783366600695,2.8116729068840409]
["Organic Carbon (TOC)",0,0,0,0,0,0,0.218,0,0]
["Apatite",0,0,0,0,0,0,0,0.89982036529533038,0]
["Pyrite",0,0,0,0,0,0,0,0,0]
["Calcite",5.9746748848631439,9.5626692644964972,0.30647272024496819,0.14422305274414005,0,0,0,0,0.22019208806413909]
["Dolomite",90.706531472634055,57.363866224232929,0.23521823060091937,0.27552020232161101,0,7.9086845760030942,0,4.6905477951843162,0.25258955547370682]
["Siderite",0,0.27505770925968642,0.18285164243651858,0.47403386081813925,0,3.4190867263722384,0,3.3531184984817686,0]
["Halite",0,0,0.52709871261621033,0.11152044643950867,0.1031682786778139,0.14953961059138407,0,0.2656409507324467,0.10046121763325465]
["TOTAL",{"$f":"SUM(B9:B18)","v":100.00000000000001},{"$f":"SUM(C9:C18)","v":94.184614391677727},{"$f":"SUM(D9:D18)","v":88.043842094704118},{"$f":"SUM(E9:E18)","v":85.697491709519525},{"$f":"SUM(F9:F18)","v":81.642457345616648},{"$f":"SUM(G9:G18)","v":81.733216064656432},{"$f":"SUM(H9:H18)","v":27.01519487535408},{"$f":"SUM(I9:I18)","v":81.459203283919194},{"$f":"SUM(J9:J18)","v":81.910463529562051}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",0,0.52935697329118947,0.23336528269422735,0.35792259549799826,0.81889633594594791,0.75926708886142313,5.5957150818077492,0.95432301540240327,1.0258549206005816]
["Illite+Mica",0,4.8219981318051648,7.6316993056199056,9.0332012841031535,11.070626877593231,11.46127015765857,56.486829185399216,10.820832159667733,10.438046472619167]
["Chlorite",0,0,1.7655692914494923,3.0434292121711413,4.7491987495340657,3.8228504930596467,7.7262454622586034,4.6645554042721971,4.6857769657234174]
["Kaolinite",0,0.46403050322590894,2.3255240255322591,1.8679551987081731,1.7188206913101032,2.2233961957639461,3.1760153951803489,2.1010861367384579,1.9398581114947862]
["TOTAL",{"$f":"SUM(B22:B25)","v":0},{"$f":"SUM(C22:C25)","v":5.8153856083222637},{"$f":"SUM(D22:D25)","v":11.956157905295884},{"$f":"SUM(E22:E25)","v":14.302508290480466},{"$f":"SUM(F22:F25)","v":18.357542654383348},{"$f":"SUM(G22:G25)","v":18.266783935343586},{"$f":"SUM(H22:H25)","v":72.984805124645902},{"$f":"SUM(I22:I25)","v":18.540796716080791},{"$f":"SUM(J22:J25)","v":18.089536470437952}]
[]
["GRAND TOTAL",{"$f":"B26+B19","v":100.00000000000001},{"$f":"C26+C19","v":99.999999999999986},{"$f":"D26+D19","v":100},{"$f":"E26+E19","v":99.999999999999986},{"$f":"F26+F19","v":100},{"$f":"G26+G19","v":100.00000000000001},{"$f":"H26+H19","v":99.999999999999986},{"$f":"I26+I19","v":99.999999999999986},{"$f":"J26+J19","v":100}]
[]
["% Expandable Layers in I/S","n/a",15.695033032800007,15.30642702839998,18.169839692400046,12.13622015040005,15.695033032800007,12.511190856399935,15.695033032800007,20.351487436400021]
["% I/S to Illite in <1.0um Fraction",0,10.877761975496139,4.9404860841793905,7.5913527743653395,11.174111011149408,10.877761975496139,14.315225211863259,10.877761975496139,16.367634795923294]
["% Expandable I/S Layers in sample","n/a",8.308275181948252E-2,3.5719886705211236E-2,6.5033961824863762E-2,9.9383062133959796E-2,0.11916722040397934,0.70162012553899811,0.14978131250702029,0.20877673528171872]
[]
["% Fe in 1st/primary Dolomite/Ankerite",27.929560699998547,45.605273399999533,null,null,null,30.668051399999968,null,29.92119029999958]
["% Fe in 2nd Dolomite/Ankerite",null,null,null,null,null,89.919032000000698,null,87.429494999999406]
[]
["Comments"]
[]
[]
["Some samples did not have enough resolution with normal XRD runs to determine"]
["clay expandability. For these samples, approximate average was used (highlighted in orange)."]