{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TOC RE6 Data","Sheet1","Pyrograms"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TOC RE6 Data","index":0,"n_rows":35,"n_cols":15,"rows_kept":35,"cut":false,"hidden":false,"merged":[[10,1,11,3],[32,0,32,5],[31,0,31,5],[10,5,11,13],[0,0,0,14],[18,0,23,0]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / RE6"]
[]
["Job Number:","15-0601"]
["Well Name:","Berea Project - F D CALDWELL ET AL 42 #465"]
["Formation:","Berea / Cleaveland / Sunberry"]
["Sample Type:","cuttings"]
["Sample Size:","20/40 mesh"]
["Instrumentation:","LECO C230 & Rock-Eval 6"]
[]
[]
[null,"Total Organic Carbon (TOC) Reference Standard Results",null,null,null,"Rock-Eval 6 (RE6) Reference Standard Results (IFP 160000)"]
[]
[null,"Date","TOC Result","% Recovery",null,"Date","S1 Result","S2 Result","S3 Result","Tmax Result","S1 % Recovery","S2 % Recovery","S3 % Recovery","Tmax % Recovery"]
[null,"2015-06-16",5.83,{"$f":"(C14/5.85)*100","v":99.658119658119674},null,"2015-06-18",0.15,12.63,0.86,415,{"$f":"(G14/0.14)*100","v":107.14285714285714},{"$f":"(H14/12.43)*100","v":101.60901045856798},{"$f":"(I14/0.79)*100","v":108.86075949367088},{"$f":"(J14/416)*100","v":99.759615384615387}]
[]
[]
[]
["DATE","Depth Range","Ave. Depth","SAMPLE ID","S1 (mg/g)","S2 (mg/g)","S3 (mg/g)","Tmax (°C)","S1+S2","Calc. %Ro-Tmax","TOC (% wt)","HI","OI","PI","NOC"]
["2015-06-18","1823-1831",1827,1,0.3,1.96,0.57999999999999996,434,2.2599999999999998,0.65199999999999925,1.79,109.49720670391061,32.402234636871505,0.13274336283185842,16.759776536312849]
[null,"1831-1839",1835,2,0.74,6.93,0.85,435,7.67,0.66999999999999904,4,173.25,21.25,9.647979139504563E-2,18.5]
[null,"1839-1850",1844.5,3,0.66,7.79,0.85,429,8.4499999999999993,0.56199999999999939,3.62,215.19337016574585,23.480662983425411,7.8106508875739653E-2,18.232044198895029]
[null,"1956-1962",1959,4,0.9,15.4,0.61,446,16.3,0.86799999999999855,3.58,430.1675977653631,17.039106145251395,5.5214723926380369E-2,25.139664804469277]
[null,"1962-1970",1966,5,0.83,13.3,0.52,445,14.13,0.84999999999999964,3.76,353.72340425531917,13.829787234042554,5.874026893135173E-2,22.074468085106382]
[null,"1970-1978",1974,6,0.95,16.420000000000002,0.55000000000000004,445,17.37,0.84999999999999964,3.32,494.57831325301214,16.566265060240966,5.4691997697179036E-2,28.614457831325304]
[]
[]
["RE6 analysis not performed on samples with TOC values < 1.50%"]
["S1 = Volatile Total Petroleum Hydrocarbons (mg/g)"]
["S2 = Kerogen yield (mg/g)"]
["HI = Hydrogen Index"]
["PI = Production Index"]
["Calc. %Ro-Tmax = Calculated%VRo = 0.0180 x Tmax - 7.16 (Jarvie et al., 2001)"]
["NOC = Normalized Oil Content = (S1/TOC) x 100 (Jarvie and Baker, 1984)"]
[]
["LECO A"]

{"sheet":"Sheet1","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":true,"merged":[[0,1,0,2],[5,1,5,2],[10,1,10,2],[15,1,15,2]]}
[null,"HI 700 LINE"]
[null,"y","x"]
[null,0,0]
[null,300,42.85]
[]
[null,"HI 350 LINE"]
[null,"y","x"]
[null,0,0]
[null,280,80]
[]
[null,"HI 200 LINE"]
[null,"y","x"]
[null,0,0]
[null,160,80]
[]
[null,"HI 50 LINE"]
[null,"y","x"]
[null,0,0]
[null,40,80]

{"sheet":"Pyrograms","index":2,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / SRA"]
[]
["Job Number:",{"$f":"'TOC RE6 Data'!B3","v":"15-0601"}]
["Well Name:",{"$f":"'TOC RE6 Data'!B4","v":"Berea Project - F D CALDWELL ET AL 42 #465"}]
["Formation:",{"$f":"'TOC RE6 Data'!B5","v":"Berea / Cleaveland / Sunberry"}]
["Sample Type:",{"$f":"'TOC RE6 Data'!B6","v":"cuttings"}]
["Sample Size:",{"$f":"'TOC RE6 Data'!B7","v":"20/40 mesh"}]