{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - F D Caldwell et al 42 465"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6"]
["SAMPLE DEPTH","1823-1831","1831-1839","1839-1850","1956-1962","1962-1970","1970-1978"]
[]
["NON-CLAY FRACTION"]
["Quartz",29.870876350581739,28.6544009116292,26.19073209311043,32.142935237747551,33.575486292821623,37.571974371243428]
["K-Feldspar",0.2282788556347424,0.28673177781058301,0.12878433105713505,0.12857408889728431,0.12288531309917368,0.12738793870583084]
["Plagioclase",4.004973159882387,4.119157865369103,3.5693660526252904,4.9412984175015291,5.8820598161188009,5.6483101318116269]
["Organic Carbon (TOC)",1.79,4,3.62,3.58,3.76,3.32]
["Apatite",0,0,0,0,0,0]
["Pyrite",2.2273330102974382,1.4157286735556054,2.7979868637242835,1.2407818034800988,1.4037886142565579,1.2929098187913932]
["Marcasite",0,0,3.9465452689607612E-2,0,0,0]
["Calcite",0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0]
["Siderite",0.34755808264414345,0.23365912346860229,0.39122309583263815,0.27302880404633267,0.58167604127371508,0.3205543180120316]
["Gypsum",0.38104370460251391,0.58101547786547025,0.44273094790367129,0,0,0]
["Anatase",0.49752047330063787,0.37855597624221643,0.4679433195921498,0.49600904593543582,0.66646431459096112,0.49623999351903147]
["Jarosite",1.0679312303661037,0.54016573953577318,1.4277551697420467,0,0,0]
["TOTAL",{"$f":"SUM(B9:B21)","v":40.415514867309703},{"$f":"SUM(C9:C21)","v":40.20941554547656},{"$f":"SUM(D9:D21)","v":39.07598732627725},{"$f":"SUM(E9:E21)","v":42.802627397608227},{"$f":"SUM(F9:F21)","v":45.992360392160826},{"$f":"SUM(G9:G21)","v":48.777376572083341}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",16.587929180247986,14.776964092530994,13.821505903900723,6.6980717047152618,8.8546006868211435,5.6886049369819096]
["Illite+Mica",36.634119536737025,42.057246845413161,43.062322602929015,44.882133850703326,39.099817542359752,39.181056920187309]
["Chlorite",2.1849430279488784,1.400417167745118,1.7617204388940699,3.3006343928601072,3.2093163270470142,3.5865175612748081]
["Kaolinite",4.1774933877564182,1.5559563488341774,2.2784637279989433,2.3165326541130811,2.8439050516112658,2.7664440094726328]
["TOTAL",{"$f":"SUM(B25:B28)","v":59.584485132690311},{"$f":"SUM(C25:C28)","v":59.790584454523454},{"$f":"SUM(D25:D28)","v":60.924012673722743},{"$f":"SUM(E25:E28)","v":57.197372602391773},{"$f":"SUM(F25:F28)","v":54.007639607839174},{"$f":"SUM(G25:G28)","v":51.222623427916666}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":100.00000000000001},{"$f":"C29+C22","v":100.00000000000001},{"$f":"D29+D22","v":100},{"$f":"E29+E22","v":100},{"$f":"F29+F22","v":100},{"$f":"G29+G22","v":100}]
[]
["% Expandable Layers in I/S",10.806778556399991,12.102131904400039,10.465896096400115,15.442780012400021,13.908808942399901,14.761015092400044]
["% I/S to Illite in <1.0um Fraction",34.508151958868474,27.320708022135737,25.754384216499982,14.590604664581811,20.897826939013182,14.855357824654927]
["% Expandable I/S Layers in sample",1.8252935277485549,1.8628413395249279,1.500876163996739,1.0727737797469299,1.2796856734646533,0.86853106464099483]
[]
["Comments"]