{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":5,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - L E Mossor 1 940"]
["JOB #","15-0601"]
["SAMPLE ID","1","2"]
["SAMPLE DEPTH","1906-1917","1951-1965"]
[]
["NON-CLAY FRACTION"]
["Quartz",39.338450445329826,38.952979077007456]
["K-Feldspar",0.34663661696799125,0.15458938577106676]
["Plagioclase",5.7997109285988593,6.1887507751935402]
["Organic Carbon (TOC)",5.65,3.58]
["Apatite",5.5134887161722296E-2,5.1336404129909786E-2]
["Pyrite",1.6348148047605719,1.6729360057976108]
["Marcasite",0,0]
["Calcite",0,0]
["Dolomite",0,0]
["Siderite",0.12900547403960425,0.20011400650736624]
["Gypsum",0.34785599634371273,0.29316284659249153]
["Anatase",0.38344504565507959,0.41503274390545558]
["TOTAL",{"$f":"SUM(B9:B20)","v":53.685054198857365},{"$f":"SUM(C9:C20)","v":51.508901244904898}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",5.091096637283413,7.3165538310238416]
["Illite+Mica",37.506169020740245,37.8362210467618]
["Chlorite",1.9813354827641474,1.7827755760841786]
["Kaolinite",1.7363446603548229,1.5555483012252946]
["TOTAL",{"$f":"SUM(B24:B27)","v":46.314945801142628},{"$f":"SUM(C24:C27)","v":48.491098755095109}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":100},{"$f":"C28+C21","v":100}]
[]
["% Expandable Layers in I/S",12.613455594399966,13.874720696400004]
["% I/S to Illite in <1.0um Fraction",14.130072496686005,18.368312801444603]
["% Expandable I/S Layers in sample",0.68061813843320929,1.0528431950386974]
[]
[]
["Comments"]