{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["TOC RE6 Data","Sheet1","Pyrograms"],"not_rendered":{"charts":0,"images":3,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"TOC RE6 Data","index":0,"n_rows":37,"n_cols":15,"rows_kept":37,"cut":false,"hidden":false,"merged":[[10,1,11,3],[34,0,34,5],[33,0,33,5],[10,5,11,13],[0,0,0,14],[18,0,25,0]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / RE6"]
[]
["Job Number:","15-0601"]
["Well Name:","Berea Project - COLUMBIA GAS 1 #1691"]
["Formation:","Berea / Cleaveland / Sunberry"]
["Sample Type:","cuttings"]
["Sample Size:","20/40 mesh"]
["Instrumentation:","LECO C230 & Rock-Eval 6"]
[]
[]
[null,"Total Organic Carbon (TOC) Reference Standard Results",null,null,null,"Rock-Eval 6 (RE6) Reference Standard Results (IFP 160000)"]
[]
[null,"Date","TOC Result","% Recovery",null,"Date","S1 Result","S2 Result","S3 Result","Tmax Result","S1 % Recovery","S2 % Recovery","S3 % Recovery","Tmax % Recovery"]
[null,"2015-06-16",5.83,{"$f":"(C14/5.85)*100","v":99.658119658119674},null,"2015-06-20",0.16,12.9,0.9,415,{"$f":"(G14/0.14)*100","v":114.28571428571428},{"$f":"(H14/12.43)*100","v":103.78117457763476},{"$f":"(I14/0.79)*100","v":113.9240506329114},{"$f":"(J14/416)*100","v":99.759615384615387}]
[]
[]
[]
["DATE","Depth Range","Ave. Depth","SAMPLE ID","S1 (mg/g)","S2 (mg/g)","S3 (mg/g)","Tmax (°C)","S1+S2","Calc. %Ro-Tmax","TOC (% wt)","HI","OI","PI","NOC"]
["2015-06-20","2170-2180",2175,1,null,null,null,null,null,null,1.3]
[null,"2180-2190",2185,2,0.09,1.34,0.8,431,1.4300000000000002,0.59799999999999898,1.9,70.526315789473685,42.10526315789474,6.2937062937062929E-2,4.7368421052631584]
[null,"2190-2200",2195,3,0.31,3.73,0.6,432,4.04,0.61599999999999966,2.02,184.65346534653466,29.702970297029701,7.6732673267326731E-2,15.346534653465346]
[null,"2200-2210",2205,4,0.76,21.84,1.2,427,22.6,0.52599999999999891,6.38,342.31974921630092,18.808777429467085,3.3628318584070796E-2,11.912225705329153]
[null,"2340-2350",2345,5,1.07,20.47,0.66,440,21.54,0.7599999999999989,3.67,557.76566757493185,17.983651226158042,4.9675023212627671E-2,29.155313351498641]
[null,"2350-2360",2355,6,0.9,16.23,0.49,440,17.13,0.7599999999999989,3.73,435.12064343163541,13.136729222520108,5.2539404553415069E-2,24.128686327077748]
[null,"2360-2370",2365,7,1.1299999999999999,20.34,0.52,442,21.47,0.79599999999999937,4.0999999999999996,496.09756097560978,12.682926829268293,5.2631578947368418E-2,27.560975609756099]
[null,"2370-2380",2375,8,1.1499999999999999,22.42,0.49,442,23.57,0.79599999999999937,4.63,484.23326133909291,10.583153347732182,4.8790835808230799E-2,24.838012958963283]
[]
[]
["RE6 analysis not performed on samples with TOC values < 1.50%"]
["S1 = Volatile Total Petroleum Hydrocarbons (mg/g)"]
["S2 = Kerogen yield (mg/g)"]
["HI = Hydrogen Index"]
["PI = Production Index"]
["Calc. %Ro-Tmax = Calculated%VRo = 0.0180 x Tmax - 7.16 (Jarvie et al., 2001)"]
["NOC = Normalized Oil Content = (S1/TOC) x 100 (Jarvie and Baker, 1984)"]
[]
["LECO B"]

{"sheet":"Sheet1","index":1,"n_rows":19,"n_cols":3,"rows_kept":19,"cut":false,"hidden":true,"merged":[[0,1,0,2],[5,1,5,2],[10,1,10,2],[15,1,15,2]]}
[null,"HI 700 LINE"]
[null,"y","x"]
[null,0,0]
[null,300,42.85]
[]
[null,"HI 350 LINE"]
[null,"y","x"]
[null,0,0]
[null,280,80]
[]
[null,"HI 200 LINE"]
[null,"y","x"]
[null,0,0]
[null,160,80]
[]
[null,"HI 50 LINE"]
[null,"y","x"]
[null,0,0]
[null,40,80]

{"sheet":"Pyrograms","index":2,"n_rows":7,"n_cols":2,"rows_kept":7,"cut":false,"hidden":false,"merged":[[0,0,0,16]]}
["CHESAPEAKE ENERGY CORPORATION - TOC / SRA"]
[]
["Job Number:",{"$f":"'TOC RE6 Data'!B3","v":"15-0601"}]
["Well Name:",{"$f":"'TOC RE6 Data'!B4","v":"Berea Project - COLUMBIA GAS 1 #1691"}]
["Formation:",{"$f":"'TOC RE6 Data'!B5","v":"Berea / Cleaveland / Sunberry"}]
["Sample Type:",{"$f":"'TOC RE6 Data'!B6","v":"cuttings"}]
["Sample Size:",{"$f":"'TOC RE6 Data'!B7","v":"20/40 mesh"}]