{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":9,"rows_kept":37,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - Columbia Gas 1 1691"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5","6","7","8"]
["SAMPLE DEPTH","2170-2180","2180-2190","2190-2200","2200-2210","2340-2350","2350-2360","2360-2370","2370-2380"]
[]
["NON-CLAY FRACTION"]
["Quartz",25.624416138502092,25.652086673568299,24.331944894405733,24.746307587880697,34.471939023665293,39.121855165656228,42.167205113690123,39.923602323358352]
["K-Feldspar",1.0004538722977816,0.79498615203730205,0.8984034652652203,0.41041413859158737,0.31389467435127238,0.22293891851217959,0.20907623895274383,0.66637114793946206]
["Plagioclase",2.6940843530912018,3.1322696144550037,3.2349307396626252,3.2863004268502247,4.905951911900428,5.9450760149184685,6.8935715640524231,6.5699603324557367]
["Organic Carbon (TOC)",1.3,1.9,2.02,6.38,3.67,3.73,4.0999999999999996,4.63]
["Apatite",0.33928570933290692,0.21747041017394297,0,1.0725143335764029,0,8.0282747374964505E-2,0,0]
["Pyrite",2.3498898624380855,3.2582294311424072,3.2927758108523562,5.5442419314348204,1.7877141730967483,1.7145423759007583,1.4906321248579826,1.8883001210207333]
["Marcasite",0,0,0,0,0,0,0,0]
["Calcite",1.3193191231458516,0,0,0,0,0,0,0]
["Dolomite",0,0,0,0,0,0,0.41436424500674429,0]
["Siderite",0,0.54905953220637471,0.23056225871855779,0.39981054397363192,0.77404911652593233,0,0,0]
["Gypsum",0.39771415832792356,0.34223536155586182,0.27160333115925073,0,0.2629399973880383,0,0,0]
["Anatase",0.74180084715531047,0.62938003074493865,0.75362325602394065,0.42287968596878811,0.6288147747193672,0.40979018639225323,0.36704389150492694,0.4282926318325852]
["TOTAL",{"$f":"SUM(B9:B20)","v":35.766964064291152},{"$f":"SUM(C9:C20)","v":36.475717205884138},{"$f":"SUM(D9:D20)","v":35.033843756087684},{"$f":"SUM(E9:E20)","v":42.262468648276148},{"$f":"SUM(F9:F20)","v":46.815303671647079},{"$f":"SUM(G9:G20)","v":51.224485408754845},{"$f":"SUM(H9:H20)","v":55.641893178064947},{"$f":"SUM(I9:I20)","v":54.106526556606873}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",8.8369937977358006,9.6143102975179815,9.7466941875364146,11.461570358878364,5.4282273752969852,5.7278473946261492,7.4491919510473377,6.2496493320788282]
["Illite+Mica",48.539730871014214,46.844153822650917,48.315732005635418,42.440292034476649,39.147807820449714,39.081229134373849,32.739017601356736,35.556266740865063]
["Chlorite",3.2480421120106517,2.4658649378013449,2.2872412788555891,2.064223315138654,3.5028167436996513,2.0783533735782345,2.1077941380764931,2.2626704358852865]
["Kaolinite",3.6082691549481694,4.5999537361456495,4.6164887718849146,1.7714456432301759,5.1058443889065606,1.8880846886669111,2.0621031314544815,1.8248869345639405]
["TOTAL",{"$f":"SUM(B24:B27)","v":64.233035935708841},{"$f":"SUM(C24:C27)","v":63.524282794115891},{"$f":"SUM(D24:D27)","v":64.966156243912337},{"$f":"SUM(E24:E27)","v":57.737531351723838},{"$f":"SUM(F24:F27)","v":53.184696328352913},{"$f":"SUM(G24:G27)","v":48.775514591245141},{"$f":"SUM(H24:H27)","v":44.358106821935053},{"$f":"SUM(I24:I27)","v":45.893473443393113}]
[]
["GRAND TOTAL",{"$f":"B28+B21","v":100},{"$f":"C28+C21","v":100.00000000000003},{"$f":"D28+D21","v":100.00000000000003},{"$f":"E28+E21","v":99.999999999999986},{"$f":"F28+F21","v":100},{"$f":"G28+G21","v":99.999999999999986},{"$f":"H28+H21","v":100},{"$f":"I28+I21","v":99.999999999999986}]
[]
["% Expandable Layers in I/S",19.056134088400086,18.885692858400034,21.408223062399998,15.170074044400053,12.033955412400019,20.21513445239998,21.987723244400058,21.885458506400141]
["% I/S to Illite in <1.0um Fraction",19.760105076807033,19.965760661724971,19.177763176833949,23.258101501827525,15.415308414031712,14.746115412604519,21.355928725630555,17.746106502608008]
["% Expandable I/S Layers in sample",1.7061695921784534,1.8508961399008894,2.1296121993037054,1.8572193015305027,0.67811736948710799,1.2027548063279996,1.7079329615645611,1.4341663115944487]
[]
[]
["Comments"]