{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
["WEIGHT PERCENT",null,null,null,"Raw Data NORMALIZED to sum to 100%"]
[]
["WELL NAME","Berea  Project - B Staley  1722"]
["JOB #","15-0601"]
["SAMPLE ID","1","2","3","4","5"]
["SAMPLE DEPTH","1850-1860","1860-1870","1870-1880","2030-2040","2050-2060"]
[]
["NON-CLAY FRACTION"]
["Quartz",32.221612500668172,34.200699715221994,31.762718528469925,32.980438113308651,25.56840779441448]
["K-Feldspar",0.65644286189094292,1.6822211856731999,0.36803269633892849,0.31788591577856379,0.39387117528268029]
["Plagioclase",3.336374856956779,3.9370929539750472,3.5486641066375029,5.1040093734750052,3.3278392326518409]
["Organic Carbon (TOC)",0.77400000000000002,0.79,1.1100000000000001,1.41,1.66]
["Apatite",0.42022218159422814,0.68584835760309137,2.6122985188355055E-2,0,0]
["Pyrite",0.37043562672655028,0.33366584606853394,0,1.9649191529087371,1.2175869567037969]
["Marcasite",0,0,0,0,0]
["Calcite",1.564637839711269,1.1865244886350395,1.1438228754289275,0.36463359186816835,1.6671669241839009]
["Dolomite",0.29908573607217365,0,0,0,0.41774240333451979]
["Siderite",4.9104441859731125,3.5828014936154693,2.846389068198075,0.18022611867408886,0.26948358584039722]
["Gypsum",0,0,0,0.55666190918049641,0.753805421257703]
["Anatase",0.65276683817247338,0.71389896787173135,0.85219529080360046,0.44637787944261742,0.50516743993631141]
["Jarosite",0,0,0,2.2469092965015687,1.6330259458724607]
["TOTAL",{"$f":"SUM(B9:B21)","v":45.206022627765705},{"$f":"SUM(C9:C21)","v":47.1127530086641},{"$f":"SUM(D9:D21)","v":41.657945551065318},{"$f":"SUM(E9:E21)","v":45.572061351137897},{"$f":"SUM(F9:F21)","v":37.414096879478087}]
[]
["CLAY FRACTION"]
["Mixed-Layer ILLITE/SMECTITE  (Includes R3)",6.2361601909939202,2.9669136227130299,5.4072121284796673,4.0781545738738423,5.0675577981455184]
["Illite+Mica",35.373701966525644,37.034079642685185,41.764499275111817,44.4140136189015,52.778299115344538]
["Chlorite",4.5875879424217016,4.6798255853618151,4.3891297299896248,1.5590593745833468,1.6994598330706698]
["Kaolinite",8.5965272722930308,8.2064281405758699,6.7812133153535763,4.376711081503398,3.040586373961192]
["TOTAL",{"$f":"SUM(B25:B28)","v":54.793977372234295},{"$f":"SUM(C25:C28)","v":52.8872469913359},{"$f":"SUM(D25:D28)","v":58.34205444893469},{"$f":"SUM(E25:E28)","v":54.427938648862082},{"$f":"SUM(F25:F28)","v":62.585903120521913}]
[]
["GRAND TOTAL",{"$f":"B29+B22","v":100},{"$f":"C29+C22","v":100},{"$f":"D29+D22","v":100},{"$f":"E29+E22","v":99.999999999999972},{"$f":"F29+F22","v":100}]
[]
["% Expandable Layers in I/S",17.760780740400037,16.77222160640008,14.692838600400023,23.214900100400087,26.555548208400069]
["% I/S to Illite in <1.0um Fraction",17.883607448436262,8.8321378096497476,12.741318585301446,9.204921922632872,9.8305092031854695]
["% Expandable I/S Layers in sample",1.1162303611377487,0.50157980815633718,0.80339058632700178,0.96027945051699914,1.368433754398078]
[]
[]
["Comments"]